>> MIB - Management Information Base
>> Table: hwAccelChanDirStatTable - (.1.3.6.1.4.1.272.4.63.1.4.1)
Description: This object contains the directional statistic info for a HW accelerator channel.
hwAccelChanDirStatTable
OID | Name | Type | Access
.1 | Slot | INTEGER | R
.2 | Unit | INTEGER | R
.3 | Chan | INTEGER | R
.4 | Direction | ENUM | R
.5 | Pkts | Counter32 | R
.6 | Path1Pkts | Counter32 | R
.7 | Path2Pkts | Counter32 | R
.12 | DiscardedPkts | Counter32 | R
.13 | LastDiscarded | TimeTicks | R
.14 | ErrorPkts | Counter32 | R
.15 | LastError | TimeTicks | R
.16 | Descrs | INTEGER | R
.17 | CurrBusyDescrs | Gauge32 | R
.18 | MaxBusyDescrs | Counter32 | R
.19 | Overflows | Counter32 | R
.20 | LastOverflow | TimeTicks | R
Slot
The slot number of this HW accelerator direction entry.
Unit
The unit number of this HW accelerator direction entry.
Chan
The channel number of this HW accelerator direction entry.
Direction
The encryption direction of this HW accelerator channel direction entry. Enumerations: decryption (1) encryption (2)
Pkts
The total number of packets for this HW accelerator channel direction.
Path1Pkts
The total number of packets for this HW accelerator channel direction seen for path 1.
Path2Pkts
The total number of packets for this HW accelerator channel direction seen for path 2.
DiscardedPkts
The total number of packets discarded due to resource problems for this HW accelerator channel direction.
LastDiscarded
The time passed since the last packet was discarded for this HW accelerator channel direction.
ErrorPkts
The number of packets which caused errors on this HW accelerator channel direction.
LastError
The time passed since the last erroneous packet on this HW accelerator channel direction.
Descrs
The number of descriptors for this HW accelerator channel direction.
CurrBusyDescrs
The number of descriptors currently in use for this HW accelerator channel direction.
MaxBusyDescrs
The maximum number of descriptors in use for this HW accelerator channel direction.
Overflows
The number of times packets were discarded because no free descriptor was found for this HW accelerator channel direction.
LastOverflow
The time passed since the last descriptor overflow occured for this HW accelerator channel direction.

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH