>> MIB - Management Information Base
>> Table: systemPhoneCapabilityTable - (.1.3.6.1.4.1.272.4.64.3.1.1)
Description: This table contains system phone capabilities which could be partially specific to phone types (for example the availability of MSN).
systemPhoneCapabilityTable
OID | Name | Type | Access
.1 | DeviceType | ENUM | R
.2 | AvailableMSN | INTEGER | R
.3 | General | BITS | R
.4 | AvailableFunctionKeys | INTEGER | R
.5 | AvailableExtFunctionKeys | INTEGER | R
.6 | MaxExtensionModules | INTEGER | R
.7 | AvailableLanguages | BITS | R
DeviceType
Subscripted via the device type of a system phone. Enumerations: cs290 (20) cs410 (22) cs290u (23) cs410u (24) cs400 (25) ips290 (32) ips400 (33) ips290plus (34) s530 (64) s560 (65) ost-40 (144) ost-80 (145) ip120 (160) ip140 (161) dect150 (162) dect200-b (163) dect200-m (164) ip130 (165) de310-ip-pro (176) de410-ip-pro (177) de700-ip-pro (178) de900-ip-pro (179) n510-ip-pro (180) n720-ip-pro (181) n720-dm-pro (182)
AvailableMSN
Number of MSNs available in this device.
General
Capabilities of different system phone types. Feature is supported by the phone device type if the BIT is set to 1: do-not-disturb: DND - Modus available. hands-free: Hands free calling possible, cause a mic in system phone integrated. local-phonebook: Has a local phonebook. intercom: Intercom available. hotel: Hotel funct./hotelroom keys available. macrokey: Macro key supported. boss-secretary: Boss-Secretary functions incl. Diversionkey available. key-extension-module: Has Key-extensions (T400, T400/2, T500). ab-module: Answering machine (module) available. headset-auto-call: (0) Auto-Call-Acceptance (key) available only if headset control (key) is set, (1) Auto-Call-Acceptance available (also without headset control (key), via hands-free telephone). extended-status-led: (0) CS/IP system phones don't support the extended status led configuration, (1) NG phones have a bitfield to configure status led on different events (eg. incoming/missing call or message). conver-disp-settings: (1) Conversation display settings are available (for CS/IP system phones), (0) NG system phones don't support this settings. ng-do-not-disturb: Special Do not disturb settings in GUI for NG system phones is enabled. Furthermore, if this bit is set a do not disturb function key is available. extended-auto-pick-up: (0) For CS/IP system phones only the following values are available for systemPhoneFacAutoCallAcceptTime: immediatly, sec-5, sec-10, (1) For NG system phones further values are available: off, sec-15, sec-20. shift-key: Shift key is available. parallel-ringing-key: Parallel ringing key available. headset-key: Headset key available. Note: NG system phones have their own firmly integrated headset key, so there is no use of this function key. connection-key: Connection keys available. Note: NG system phones don't support this kind of key. Enumerations: do-not-disturb (0) hands-free (1) local-phonebook (2) intercom (3) hotel (4) macrokey (5) boss-secretary (6) key-extension-module (7) ab-module (8) headset-auto-call (9) extended-status-led (10) conver-disp-settings (11) ng-do-not-disturb (12) extended-auto-pick-up (13) shift-key (14) parallel-ringing-key (15) headset-key (16) connection-key (17)
AvailableFunctionKeys
Number of (2-level) function keys available on this device.
AvailableExtFunctionKeys
Number of function keys available on the expansion module.
MaxExtensionModules
Maximum number of key expansion modules which can be connected to this device.
AvailableLanguages
A matrix of supported display languages by the phone device. Enumerations: german (1) dutch (2) english (3) italian (5) danish (6) spanish (7) swedish (8) french (10) portuguese (11) czech (14) norwegian (16) greek (17) icelandic (20) polish (21) hungarian (22) russian (23) romanian (24) slovak (25)

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH