>> MIB - Management Information Base
>> Table: wlcScanResultsTable - (.1.3.6.1.4.1.272.4.61.1.27.1)
Description: This table contains the list of BSS entries found by foreground or background scanning.
wlcScanResultsTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | wlanIfIndex | INTEGER | R
.3 | BSSID | MacAddress | R
.4 | RSSI | WlanRSSI | R
.5 | SSID | DisplayString | R
.6 | Channel | INTEGER | R
.7 | Privacy | ENUM | R
.8 | Type | ENUM | R
.9 | WPAUnicastCipher | BITS | R
.10 | RSNUnicastCipher | BITS | R
.11 | APType | ENUM | R
.12 | LastSeen | Date | R
Index
Auxiliary index for different BSS entries.
wlanIfIndex
Index of WLAN Interface the scan results belong to.
BSSID
BSSID of this BSS. Length: 6 to 6
RSSI
Receive signal strength of this BSS. Range: -110 to 0
SSID
SSID aka network name of this BSS. If broadcasting of SSID is disabled on this BSS, this string may be empty. Length: 0 to 255
Channel
The channel this BSS was received on.
Privacy
This attribute contains the privacy type of the scanned device. Enumerations: none (1) wep (2) wpa-psk (3) wpaandwpa2-psk (4) wpa2-psk (5) wpa-enterprise (6) wpaandwpa2-enterprise (7) wpa2-enterprise (8)
Type
This attribute contains the device type of the scanned device. Enumerations: access-point (1) ad-hoc (2)
WPAUnicastCipher
This attribute contains the WPA unicast ciphers of the scanned device. Enumerations: cipher-none (0) cipher-wep40 (1) cipher-wep104 (2) cipher-tkip (3) cipher-aes (4)
RSNUnicastCipher
This attribute contains the RSN unicast ciphers of the scanned device. Enumerations: cipher-none (0) cipher-wep40 (1) cipher-wep104 (2) cipher-tkip (3) cipher-aes (4)
APType
This attribute contains the type of the scanned access point. 'own' -> managed AP, 'neighborhood' -> neighborhood AP 'rogue' -> foreign AP but with one of our SSIDs, 'own-manipulated' -> managed AP but with manipulated configuration. 'knownneighbor' -> a neigborhood AP but well known by wlcKnownAPTable 'knownrogue' -> foreign AP with one of our SSIDs but is well known by wlcKnownAPTable Enumerations: own (1) neighborhood (2) rogue (3) own-manipulated (4) knownneighbor (5) knownrogue (6)
LastSeen
This attribute contains that time when an access point or client was seen for the last time. Range: 0 to -1

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH