>> MIB - Management Information Base
>> Table: mpsExtensionUserTable - (.1.3.6.1.4.1.272.4.53.6.3.1)
Description: This table contains extended settings for internal extensions.
mpsExtensionUserTable
OID | Name | Type | Access
.1 | Index | ExtensionIndex | RW
.2 | AuthPassword | DisplayString | RW
.3 | ChargeLimit | Unsigned32 | RW
.4 | DirectCall | DirectCallIndexOrZero | RW
.5 | Facilities | BITS | RW
.6 | AdminStatus | ENUM | D
.7 | UserMode | Unsigned32 | RW
Index
This variable references the mpsExtensionIndex. Range: 1 to 65535
AuthPassword
Password for VoIP-registration at the PBX. Length: 0 to 8
ChargeLimit
This variable contains the maximum amounts available for calling.
DirectCall
This variable contains the index of the DirectCallTable. 0 = disabled. Range: 0 to 65535
Facilities
Special facilities of the extension. charge-limit: This value determines if the maximum amounts available for calling is enabled. call-waiting: Call waiting signal for analog terminals. ISDN terminal devices use their own special procedures for this. announcement: Enables this phone to receive announcement calls. intercom: Allows intercom calls to the system telephone or to another identical ISDN telephone. silent-phone-intern: Enables a silent phone for incoming internal calls. silent-phone-extern: Enables a silent phone for incoming external calls. direct-call : Enables a direct call. parallel-ringing: Enables parallel ringing. Enumerations: charge-limit (0) call-waiting (1) announcement (2) intercom (3) silent-phone-intern (4) silent-phone-extern (5) direct-call (6) parallel-ringing (7)
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
UserMode
This variable contains the actual mode for the incoming call distribution to a reroute function.

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH