>> MIB - Management Information Base
>> Table: frDlcmiTable - (.1.3.6.1.2.1.10.32.1.1)
Description: The Parameters for a particular Data Link Con- nection Management Interface.
frDlcmiTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | State | ENUM | RW
.3 | Address | ENUM | RW
.4 | AddressLen | ENUM | RW
.5 | PollingInterval | INTEGER | RW
.6 | FullEnquiryInterval | INTEGER | RW
.7 | ErrorThreshold | INTEGER | RW
.8 | MonitoredEvents | INTEGER | RW
.9 | MaxSupportedVCs | INTEGER | RW
.10 | Multicast | ENUM | RW
.42 | DceIdleInterval | INTEGER | RW
.43 | DceErrorThreshold | INTEGER | RW
.44 | DceMonitoredEvents | INTEGER | RW
.45 | Mode | ENUM | RW
.46 | DefaultRouteIfIndex | INTEGER | RW
IfIndex
The ifIndex value of the corresponding ifEn- try.
State
This variable states which Data Link Connec- tion Management scheme is active (and by impli- cation, what DLCI it uses) on the Frame Relay interface. Enumerations: noLmiConfigured (1) lmiRev1 (2) ansiT1-617-D (3) ansiT1-617-B (4) q933a (5) original-lmi (6)
Address
This variable states which address format is in use on the Frame Relay interface. Enumerations: q921 (1) q922March90 (2) q922November90 (3) q922 (4)
AddressLen
This variable states which address length in octets. In the case of Q922 format, the length indicates the entire length of the address in- cluding the control portion. Enumerations: two-octets (2) three-octets (3) four-octets (4)
PollingInterval
This is the number of seconds between succes- sive status enquiry messages. Range: 5 to 30
FullEnquiryInterval
Number of status enquiry intervals that pass before issuance of a full status enquiry mes- sage. Range: 1 to 255
ErrorThreshold
This is the maximum number of unanswered Status Enquiries the equipment shall accept be- fore declaring the interface down. Range: 1 to 10
MonitoredEvents
This is the number of status polling intervals over which the error threshold is counted. For example, if within 'MonitoredEvents' number of events the station receives 'ErrorThreshold' number of errors, the interface is marked as down. Range: 1 to 10
MaxSupportedVCs
The maximum number of Virtual Circuits allowed for this interface. Usually dictated by the Frame Relay network. In response to a SET, if a value less than zero or higher than the agent's maximal capability is configured, the agent should respond bad- Value Range: 0 to 1023
Multicast
This indicates whether the Frame Relay inter- face is using a multicast service. Enumerations: nonBroadcast (1) broadcast (2)
DceIdleInterval
This is the number of seconds within a status enquiry messages should be received. Range: 10 to 60
DceErrorThreshold
This is the maximum number of unsent Status Enquiries the equipment shall accept be- fore declaring the interface down. Range: 1 to 10
DceMonitoredEvents
This is the number of status polling intervals over which the error threshold is counted. For example, if within 'MonitoredEvents' number of events the station receives 'ErrorThreshold' number of errors, the interface is marked as down. Range: 1 to 10
Mode
This indicates the mode of the interface. dte(1) does status enquiry polling, dce(2) does status answering. nni(3) is bidirectional use of both dte and dce. Enumerations: dte (1) dce (2) nni (3)
DefaultRouteIfIndex
This is the default route interface index when a new PVC is established by means of line management.

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH