>> MIB - Management Information Base
>> Table: wlcWTPInfoTable - (.1.3.6.1.4.1.272.4.61.1.23.1)
Description: The table contains different information of each WTP.
wlcWTPInfoTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | WTPIndex | INTEGER | R
.3 | MacAddress | MacAddress | R
.4 | State | ENUM | R
.5 | Device | DisplayString | R
.6 | SerialNo | DisplayString | R
.7 | SwVer | DisplayString | R
.8 | InetAddressType | ENUM | R
.9 | InetAddress | IpAddress | R
.10 | NoRadios | INTEGER | R
.11 | ConnectTime | TimeTicks | R
.12 | TxPackets | Counter32 | R
.13 | TxBytes | Counter32 | R
.14 | RxPackets | Counter32 | R
.15 | RxBytes | Counter32 | R
.16 | Retransmissions | Counter32 | R
.17 | LastSeen | Date | R
Index
Unique WTP information index.
WTPIndex
Unique WTP index.
MacAddress
The first ethernet MAC address of the WTPs. Length: 6 to 6
State
Reflects the current (CAPWAP) state of the WTP. idle(1) - WTP is idle (isn't seen by AC) discovery(2) - WTP is discovered by AC authorize(3) - WTP is waiting to be authorized by AC join(4) - WTP send join request to AC configure(5) - AC replied to join and send configure request mib-configure(6) - WTP retrieves configuration from AC data-check(7) - WTP is (re)configuring itself run(8) - WTP has finished configuration and is now managed reset(9) - WTP will be resetted (reboot). lostac(10) - The WTP lost the connection to its AC (see: wlcACLostACLifeTime) Default is idle(1). Enumerations: idle (1) discovery (2) authorize (3) join (4) configure (5) mib-configure (6) data-check (7) run (8) reset (9) lostac (10)
Device
The official WTP device name. Length: 0 to 255
SerialNo
The unique serial number of the WTP Length: 0 to 64
SwVer
Current software version of the WTP Length: 0 to 32
InetAddressType
The IP address type of the WTP. It is one of: -unknown(0): an unknown address type -ipv4(1) : an IPv4 address -ipv6(2) : an IPv6 address -ipv4z(3) : a non-global IPv4 address including a zone index -ipv6z(4) : a non-global IPv6 address including a zone index -dns(16) : a DNS domain name Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
InetAddress
IP address of the requested WTP.
NoRadios
Number of radios that the device has.
ConnectTime
This attribute records the time since last state change.
TxPackets
The transmitted packets of the requested WTP.
TxBytes
Number of transmitted bytes of the requested WTP.
RxPackets
Number of received packets of the requested WTP.
RxBytes
Number of received bytes of the requested WTP.
Retransmissions
Number of retransmissions of the requested WTP.
LastSeen
On Ac this is the timestamp of the last receved CAPWAP UDP packet from that WTP. On WTP this is the timestamp of the last received CAPWAP UDP packet from AC. Range: 0 to -1

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH