>> MIB - Management Information Base
>> Table: mpsExtensionAdminTable - (.1.3.6.1.4.1.272.4.53.6.2.1)
Description: This table contains extended settings for internal extension.
mpsExtensionAdminTable
OID | Name | Type | Access
.1 | Index | ExtensionIndex | RW
.2 | DialAuthorisation | ENUM | RW
.3 | Facilities | BITS | RW
.4 | PickupGroup | INTEGER | RW
.5 | PhonebookAccess | ENUM | RW
.6 | MusicOnHold | ENUM | RW
.7 | AdminStatus | ENUM | D
.8 | Calendar | CalendarIndexOrZero | RW
.9 | WrapUpTime | INTEGER | RW
Index
A unique value for each extension. Range: 1 to 65535
DialAuthorisation
Dialing privileges for a extension specifies what type of calls (internal, external, etc. ) this extension can place. Default is international. Enumerations: unknown (1) international (2) incoming (3) national (4) region (5) internal (6) onlyDoorIntercom (7) local (8)
Facilities
Special facilities of the extension. suppress-A-Addr: Suppress outgoing CLIP information (CLIR). suppress-B-Addr: This value determines if supression number of called party (COLR) is enabled or not. store-charge: Charge information for this subscriber will be record or not. doorIntercom-access: Authorizes an internal subscriber to establish a connection with the door entry phone or open the door. auto-trunk-req: This setting defines whether automatic access to an outside line is to be configured for the selected subscriber. keypad: Authorizes an internal subscriber to carry out KEYPAD functions. route-barring: If you have configured the dialing filter (consisting of an inhibit and release filter) in the PBX system you can use these settings to define whether the selected subscriber is subject to the constraints/ privileges imposed/offered by the dialing filter. add-trunk-acc-dig: The line access code is placed in front of the number automatically by the PBX system for incoming external calls. rma-access: This permits a subscriber to activate the service access to the PBX system, or to establish a corresponding service connection on their own. extern-diversion: You can use this setting to define whether external call forwarding for the internal subscriber is to be executed within the PBX system or at the exchange. extern-hold: You can use this setting to define whether external call hold for the internal subscriber is to be executed within the PBX system or at the exchange. add-line-acc-dig: The internal dialing code is places in front of the number automatically by the PBX system for incoming internal calls. msg-waiting: Message waiting indication on or off. time-lock: If on, the access rights will be changed at a time specified in the calendar. sms: Authorizes an internal subscriber to receive SMS messages. rma-user-access: Authorization for remote access activation is on or off. tapi: Authorizes a subscriber to use the PBX's TAPI features. ccnr: The completion of call on no answer (CCNR) feature is available to the user. showInPhonebook: Show this extension number in display at access to the global phonebook. statusLED: Show status of this extension number at status LED at systemphones. call-center-agent: Mark this extension as call center agent. . Enumerations: suppress-A-Addr (0) suppress-B-Addr (1) store-charge (2) doorIntercom-access (3) auto-trunk-req (4) keypad (5) route-barring (6) add-trunk-acc-dig (7) rma-access (8) extern-diversion (9) extern-hold (10) add-line-acc-dig (11) msg-waiting (12) time-lock (13) sms (14) rma-user-access (15) tapi (16) ccnr (17) showInPhonebook (18) statusLED (19) call-center-agent (20)
PickupGroup
Enter the number of the group in which calls are to be taken.
PhonebookAccess
This value determine the access to the PBX phonebook. Enumerations: denied (1) restricted (2) unrestricted (3)
MusicOnHold
This variable contains the selected music on hold (MoH) that a party is to hear that has been transferred by the selected internal subscriber. Enumerations: file1 (1) file2 (2) file3 (3) file4 (4) file5 (5) file6 (6) file7 (7) file8 (8) dialtone (50) default1 (51) default2 (52) external (80)
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
Calendar
Select a calendar index to switch the call distribution for rerouting via calendar. Range: 0 to 65535
WrapUpTime
This variable contains the length of timer in seconds for the wrap up time. This timer value is used, if mpsGroupModeOperation is set to 'callcenter'. Range: 0 to 999

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH