>> MIB - Management Information Base
>> Table: mpsAlarmInputTable - (.1.3.6.1.4.1.272.4.53.18.2.1)
Description: Settings for each alarm input mapped to FXS ports.
mpsAlarmInputTable
OID | Name | Type | Access
.1 | IfIndex | InterfaceIndexOrZero | RW
.2 | IndicationExtension | ExtensionIndexOrZero | RW
.3 | Contact | SwitchingContactIndexOrZero | RW
.4 | WaveType | ENUM | RW
.5 | WaveFileDir | DisplayString | RW
.6 | WaveDefaultVariant | INTEGER | RW
.7 | WavePlayBackCnt | Unsigned32 | RW
.8 | Group | GroupIndexOrZero | RW
.9 | SignalingTimer | Unsigned32 | RW
.10 | SignalingRepeat | Unsigned32 | RW
.11 | DelayTimer | Unsigned32 | RW
.12 | ExternalConnTimer | Unsigned32 | RW
.13 | InfoMsg | DisplayString | RW
.14 | AdminStatus | ENUM | D
IfIndex
A unique reference to potsIfTable. Range: 0 to 2147483647
IndicationExtension
A unique reference to mpsExtensionTable. This reference assignes the indication number of the alarm input. Range: 0 to 65535
Contact
A unique reference to mpsSwitchingContactTable. This reference assignes a relay contact which have to be switched if alarm input is initiated. Range: 0 to 2
WaveType
This variable contains the file/tone the remote is provided with, when alarm call is answered. Possible values are: file: variable mpsAlarmInputWaveDir specifies the directory that contains the sound file default: variable mpsAlarmInputWaveDefaultVariant specifies the variant whose default is to be used external: external source is used off: no wave on alarm call active (default) Enumerations: file (54) default (55) external (80) off (100)
WaveFileDir
Name of directory (on flash medium) which contains the file to be used as alarm call wave file. This variable references the entry in mpsWaveFile table where mpsWaveFileDirectory has identical content. the entry is only valid if variable mpsAlarmInputWaveType is set to value file. Default value is the empty string. Length: 0 to 255
WaveDefaultVariant
This variable specifies the chosen default variant if variable mpsAlarmInputWaveType is set to value default. Default value for that variable is 1. Range: 1 to 2
WavePlayBackCnt
Value contains number of playbacks of selected wave file. (0 = endless). Range: 0 to 10
Group
A unique reference to mpsGroupTable. This reference assignes a special group to the alarm input. All settings for call distribution of alarm input are outsourced in the mpsGroupTable and the corresponding sub-tables. Range: 0 to 99
SignalingTimer
This value contains the signaling timeout of the alarm. After expiration of this timer, the alarm call will be released and delayed for the value stored in mpsAlarmInputDelayTimer. Range: 1 to 600
SignalingRepeat
This value contains the number of signaling repetition on no response (after mpsAlarmInputSignalingTimeout expires) or all team-members are busy (and call waiting is restricted). Range: 0 to 10
DelayTimer
This value contains the delay-timer of the alarm. After expiring of this timer, the alarm call will be re-established if mpsAlarmInputSignalingRepeat-counter unequals 0. Range: 1 to 600
ExternalConnTimer
This value contains the external connection timer of the alarm. After timer expiry the external alarm call will be released. Range: 1 to 600
InfoMsg
An info message (UUS1) delivered if alarm is initiated. Terminals must support UUS1-text messages to show this info message. Length: 0 to 32
AdminStatus
Just for MIB entry deletion and for deactivation. Enumerations: enable (1) disable (2) delete (3)

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH