>> MIB - Management Information Base
>> Table: wlanClientStatsTable - (.1.3.6.1.4.1.272.4.46.25.1)
Description: Shows WLAN Client statistics
wlanClientStatsTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Bss | MacAddress | R
.3 | CurrSSID | DisplayString | R
.4 | MSDUTx | Counter32 | R
.5 | MSDURx | Counter32 | R
.6 | BytesTx | Counter32 | R
.7 | BytesRx | Counter32 | R
.8 | Rate | WlanRate | R
.9 | RSSI | WlanRSSI | R
.10 | Noise | WlanRSSI | R
.11 | RxFrames54 | Counter32 | R
.12 | RxFrames48 | Counter32 | R
.13 | RxFrames36 | Counter32 | R
.14 | RxFrames24 | Counter32 | R
.15 | RxFrames18 | Counter32 | R
.16 | RxFrames12 | Counter32 | R
.17 | RxFrames11 | Counter32 | R
.18 | RxFrames9 | Counter32 | R
.19 | RxFrames6 | Counter32 | R
.20 | RxFrames5 | Counter32 | R
.21 | RxFrames2 | Counter32 | R
.22 | RxFrames1 | Counter32 | R
.23 | TxFrames54 | Counter32 | R
.24 | TxFrames48 | Counter32 | R
.25 | TxFrames36 | Counter32 | R
.26 | TxFrames24 | Counter32 | R
.27 | TxFrames18 | Counter32 | R
.28 | TxFrames12 | Counter32 | R
.29 | TxFrames11 | Counter32 | R
.30 | TxFrames9 | Counter32 | R
.31 | TxFrames6 | Counter32 | R
.32 | TxFrames5 | Counter32 | R
.33 | TxFrames2 | Counter32 | R
.34 | TxFrames1 | Counter32 | R
.35 | RSSI1 | WlanRSSI | R
.36 | RSSI2 | WlanRSSI | R
.37 | RSSI3 | WlanRSSI | R
IfIndex
IfIndex of the client interface.
Bss
BSS Id the client is associated with. If client is not associated, this attribute reads 00:00:00:00:00:00.
CurrSSID
The Service Set Name the client really is associated with. This usually equal to wlanClientSSID, except for empty wlanClientSSID, which means any SSID.
MSDUTx
Count of transmitted MSDU.
MSDURx
Count of received MSDU.
BytesTx
Total number of transmitted bytes.
BytesRx
Total number of received bytes.
Rate
Data rate of latest received data frame, in 500 kbps units. If client is not associated, this attribute always reads 0.
RSSI
Receive signal strength of latest received data frame.
Noise
This attribute shows the measured noise level in dBm, or 0 if no connection can be established.
RxFrames54
This attribute shows the number of data frames that were received at 54 Mbps.
RxFrames48
This attribute shows the number of data frames that were received at 48 Mbps.
RxFrames36
This attribute shows the number of data frames that were received at 36 Mbps.
RxFrames24
This attribute shows the number of data frames that were received at 24 Mbps.
RxFrames18
This attribute shows the number of data frames that were received at 18 Mbps.
RxFrames12
This attribute shows the number of data frames that were received at 12 Mbps.
RxFrames11
This attribute shows the number of data frames that were received at 11 Mbps.
RxFrames9
This attribute shows the number of data frames that were received at 9 Mbps.
RxFrames6
This attribute shows the number of data frames that were received at 6 Mbps.
RxFrames5
This attribute shows the number of data frames that were received at 5.5 Mbps.
RxFrames2
This attribute shows the number of data frames that were received at 2 Mbps.
RxFrames1
This attribute shows the number of data frames that were received at 1 Mbps.
TxFrames54
This attribute shows the number of data frames that were transmitted at 54 Mbps.
TxFrames48
This attribute shows the number of data frames that were transmitted at 48 Mbps.
TxFrames36
This attribute shows the number of data frames that were transmitted at 36 Mbps.
TxFrames24
This attribute shows the number of data frames that were transmitted at 24 Mbps.
TxFrames18
This attribute shows the number of data frames that were transmitted at 18 Mbps.
TxFrames12
This attribute shows the number of data frames that were transmitted at 12 Mbps.
TxFrames11
This attribute shows the number of data frames that were transmitted at 11 Mbps.
TxFrames9
This attribute shows the number of data frames that were transmitted at 9 Mbps.
TxFrames6
This attribute shows the number of data frames that were transmitted at 6 Mbps.
TxFrames5
This attribute shows the number of data frames that were transmitted at 5.5 Mbps.
TxFrames2
This attribute shows the number of data frames that were transmitted at 2 Mbps.
TxFrames1
This attribute shows the number of data frames that were transmitted at 1 Mbps.
RSSI1
Receive signal strength of latest data frame received by first receiver. A value of 0 inidcates no connection.
RSSI2
Receive signal strength of latest data frame received by first receiver. A value of 0 inidcates no second receiver present or no connection.
RSSI3
Receive signal strength of latest data frame received by third receiver. A value of 0 inidcates no third receiver present or no connection.

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH