>> MIB - Management Information Base
>> Table: dot11AntennasListTable - (.1.2.840.10036.4.8.1)
Description: An entry in the dot11AntennasListTable, representing the properties of a single antenna. ifIndex - Each 802.11 interface is represented by an ifEntry. Interface tables in this MIB module are indexed by ifIndex.
dot11AntennasListTable
OID | Name | Type | Access
.1 | AntennaListIndex | Integer32 | R
.2 | SupportedTxAntenna | ENUM | RW
.3 | SupportedRxAntenna | ENUM | RW
.4 | DiversitySelectionRx | ENUM | RW
AntennaListIndex
The unique index of an antenna which is used to identify the columnar objects in the dot11AntennasList Table. Range: 1 to 255
SupportedTxAntenna
When true, this object indicates that the antenna represented by dot11AntennaIndex can be used as a transmit antenna. Enumerations: true (1) false (2)
SupportedRxAntenna
When true, this object indocates that the antenna represented by the dot11AntennaIndex xan be used as a receive antenna. Enumerations: true (1) false (2)
DiversitySelectionRx
When true, this object indicates that the antenna represented by dot11AntennaIndex can be used for receive diversity. This object may only be true if the antenna can be used as a receive antenna, as indicated by dot11SupportedRxAntenna. Enumerations: true (1) false (2)

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH