>> MIB - Management Information Base
>> Table: pppLinkHistoryTable - (.1.3.6.1.4.1.272.4.3.13.1)
Description: The pppLinkHistoryTable contains statistical information for each closed PPP link on the system. Only the system can add or delete entries to this table. Creating entries: Entries are created by the system each time a PPP link is closed. Deleting entries: Entries are removed by the system either the maximum number of entries is reached or when the corresponding PPP interface is removed.
pppLinkHistoryTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Id | INTEGER | R
.3 | Created | Date | R
.4 | Direction | ENUM | R
.9 | Accm | OCTET STRING | R
.10 | Lqm | ENUM | R
.11 | LcpComp | ENUM | R
.12 | LocDiscr | OCTET STRING | R
.13 | RemDiscr | OCTET STRING | R
.14 | LocAuth | ENUM | R
.15 | RemAuth | ENUM | R
.17 | L1Protocol | ENUM | R
IfIndex
Correlating PPP interface index.
Id
Unique ID for this entry.
Created
Time when this entry was created. Range: 0 to -1
Direction
Direction of link, incoming(1) or outgoing(2). In case of permanent links, the meaning is dce(1) or dte(2). Enumerations: incoming-dce (1) outgoing-dte (2)
Accm
The Asynchronous Control Character Map (ACCM) according RFC 1662. Length: 4 to 4
Lqm
Indicates the successful negotiation of the Link Quality Protocol (LQM). Enumerations: none (1) negotiated (2)
LcpComp
Address- and Protocol-Field compression. Enumerations: none (1) addr (2) prot (3) both (4)
LocDiscr
Local LCP multilink endpoint discriminator. Length: 6 to 6
RemDiscr
Peer's LCP multilink endpoint discriminator. Length: 20 to 20
LocAuth
The result of the PPP authentication procedure performed locally. Enumerations: none (1) successful (2) failed (3) timeout (4) prot-rejected (5)
RemAuth
The result of the PPP authentication procedure performed on remote. Enumerations: none (1) successful (2) failed (3) timeout (4) prot-rejected (5)
L1Protocol
The layer 1 protocol of this link. Enumerations: data-64k (1) data-56k (2) modem (3) dovb (4) v110-1200 (5) v110-2400 (6) v110-4800 (7) v110-9600 (8) v110-14400 (9) v110-19200 (10) v110-38400 (11) modem-profile-1 (12) modem-profile-2 (13) modem-profile-3 (14) modem-profile-4 (15) modem-profile-5 (16) modem-profile-6 (17) modem-profile-7 (18) modem-profile-8 (19) pptp-pns (20) pppoe (21) pppx25 (22) pptp-pac (23) l2tp-lns (24) l2tp-lac (25) dovb-64k (26) all (31)

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH