>> MIB - Management Information Base
>> Table: mpsUserTable - (.1.3.6.1.4.1.272.4.53.6.14.1)
Description: This table contains the information about users.
mpsUserTable
OID | Name | Type | Access
.1 | Index | UserIndex | RW
.2 | Name | DisplayString | RW
.3 | Description | DisplayString | RW
.4 | LoginUser | DisplayString | RW
.5 | MobileNumber | DisplayString | RW
.6 | HomeNumber | DisplayString | RW
.7 | MailAddress | DisplayString | RW
.8 | Facilities | BITS | RW
.9 | CallThroughOutExtIndex | ExtensionIndexOrZero | RW
.10 | StandardCoS | CoSIndexOrZero | RW
.11 | OptionalCoS | CoSIndexOrZero | RW
.12 | NightCoS | CoSIndexOrZero | RW
.13 | AuthPassword | DisplayString | RW
.14 | AdminStatus | ENUM | D
Index
A unique value for each user. Range: 1 to 65535
Name
This variable contains the name of the user. Length: 0 to 255
Description
This variable contains additional description for the user. e.g. 'Hotline' or 'R&D'. Length: 0 to 255
LoginUser
This variable contains the login user string, referencing variable biboAdmLoginUser in biboAdmLoginTable. This string will be used in mpsExtensionLoginUser, too. Length: 0 to 255
MobileNumber
This variable contains the user's mobile number. Length: 0 to 24
HomeNumber
This variable contains the user's home number. Length: 0 to 24
MailAddress
This variable contains the user's mail address. Length: 0 to 64
Facilities
user facilities. showMobilNumInPhonebook: Select whether this number is shown during system phonebook acces. showHomeNumInPhonebook: Select whether this number is shown during system phonebook acces. callThrough: Select whether call through should be authorised for this user. Enumerations: showMobilNumInPhonebook (0) showHomeNumInPhonebook (1) callThrough (2)
CallThroughOutExtIndex
This variable contains the extension index for outgoing call routing, if mpsUserFacilities callThrough option is enabled. Otherwise this value is unused. Range: 0 to 65535
StandardCoS
This variable contains the index of the standard class of service referencing mpsCoSIndex in mpsClassOfServiceTable. Range: 0 to 65535
OptionalCoS
This variable contains the index of the optional class of service referencing to mpsCoSIndex in mpsClassOfServiceTable. Range: 0 to 65535
NightCoS
This variable contains the index of the night class of service referencing to mpsCoSIndex in mpsClassOfServiceTable. Range: 0 to 65535
AuthPassword
This variable contains authorisation password used for VoIP client registration. Length: 0 to 32
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH