>> MIB - Management Information Base
>> Table: systemPhoneModuleTable - (.1.3.6.1.4.1.272.4.64.2.1.1)
Description: This table contains information about base and extension modules of system phones.
systemPhoneModuleTable
OID | Name | Type | Access
.1 | Index | SystelModuleIndex | RW
.2 | TermIndex | SystelTerminalIndex | RW
.3 | Type | ENUM | RW
.4 | Prio | INTEGER | RW
.5 | Version | DisplayString | R
.6 | RelDate | DisplayString | R
.7 | SerNum | DisplayString | RW
.8 | OperStatus | ENUM | R
.9 | AdminStatus | ENUM | D
Index
A unique value for system phone itself (base) or any extension module (e.g. T400, T400/2, T500, Answering machine). Range: 1 to 65535
TermIndex
A reference to systemPhoneTable (or mpsTerminalTable). Range: 1 to 65535
Type
The module type: base: module is the system phone itself. t400: module is a keypad extension T400. ab-mod: module is an answering machine. t400-2: module is a keypad extension T400/2. t500: module is a NG Phone keypad extension T500 giga..: module is a gigaset phone base or expansion module Enumerations: base (1) t400 (2) ab-mod (3) t400-2 (4) t500 (5) gigaset-base (6) gigaset-expansion-module (7)
Prio
The variable defines the module position docked to the base system phone. Range: 0 to 3
Version
Information about the module's software version. Length: 0 to 9
RelDate
Information about the module's release date. Length: 0 to 17
SerNum
The serial number of the module. Length: 0 to 15
OperStatus
Operational status of the module. Enumerations: connected (1) unconnected (2) unsupported (3)
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH