>> MIB - Management Information Base
>> Table: dot11RSNAConfigPairwiseCiphersTable - (.1.2.840.10036.1.10.1)
Description: The table entry, indexed by the interface index (or all interfaces) and the pairwise cipher.
dot11RSNAConfigPairwiseCiphersTable
OID | Name | Type | Access
.1 | Index | Unsigned32 | R
.2 |  | OCTET STRING | R
.3 | Enabled | ENUM | RW
.4 | Size | Unsigned32 | R
Index
The auxiliary index into the dot11RSNAConfigPairwiseCiphersTable. Range: 1 to -1
The selector of a supported pairwise cipher. It consists of an OUI (the first 3 octets) and a cipher suite identifier (the last octet). Length: 4 to 4
Enabled
This object enables or disables the pairwise cipher. Enumerations: true (1) false (2)
Size
This object indicates the length in bits of the pairwise cipher key. This should be 256 for TKIP and 128 for CCMP. Range: 0 to -1

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH