>> MIB - Management Information Base
>> Table: wlcAutoWTPTable - (.1.3.6.1.4.1.272.4.61.1.36.1)
Description: The table defines auto configuration of each WTP.
wlcAutoWTPTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | SelectorIndex | INTEGER | RW
.3 | Location | DisplayString | RW
.4 | Description | DisplayString | RW
.5 | secIndex | INTEGER | RW
.6 | localServicesIndex | INTEGER | RW
Index
Unique index.
SelectorIndex
Configured Selector index. See wlcAutoSelectorIndex.
Location
Location of the requested WTP. Length: 0 to 63
Description
Description of the requested WTP. Length: 0 to 63
secIndex
This attribute shows the currently configured secIndex of the requested WTP.
localServicesIndex
This attribute shows the currently configured localServicesIndex of the requested WTP.

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH