>> MIB - Management Information Base
>> Table: dot1dStaticAllowTable - (.1.3.6.1.4.1.272.4.8.5.1.1)
Description: Filtering information configured into the bridge by (local or network) management specifying the set of ports to which frames received from a specific port and containing a specific destination address are allowed to be forwarded.
dot1dStaticAllowTable
OID | Name | Type | Access
.1 | SrcIfIndex | INTEGER | RW
.2 | DstIfIndex | INTEGER | RW
.3 | ByteOffset | INTEGER | RW
.4 | Mask | OCTET STRING | RW
.5 | Value | OCTET STRING | RW
.6 | Status | ENUM | D
.7 | Age | TimeTicks | RW
SrcIfIndex
Either the value '0', or the port number of the port from which a frame must be received in order for this entry's filtering information to apply. A value of zero indicates that this entry applies on all ports of the bridge for which there is no other applicable entry.
DstIfIndex
Either the value '0', or the port number of the port to which a frame can be forwarded. A value of zero indicates that this entry applies on all ports of the bridge for which there is no other applicable entry.
ByteOffset
The number of bytes in the packet that are skipped before making the comparison. Range: 0 to 65535
Mask
This octet string specifies which bytes are compared. Leading 0's are handled as when using dot1dStaticAllowByteOffset. Length: 0 to 64
Value
The value of the bytes to look for. For example: Offset=12 Offset=0 Mask=ff:ff Mask=0:0:0:0:0:0:0:0:0:0:0:0:ff:ff Value=81:37 Value=0:0:0:0:0:0:0:0:0:0:0:0:81:37 Both examples above specify that the 13th byte must be '0x81' and the 14th byte must be '0x37' in order for the filter to match. These examples would allow IPX packets to be bridged. Length: 0 to 64
Status
The status of this entry. Enumerations: other (1) invalid (2) permanent (3) deleteOnReset (4) deleteOnTimeout (5)
Age
Age of the entry in seconds.

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH