>> MIB - Management Information Base
>> Table: systemPhoneTable - (.1.3.6.1.4.1.272.4.64.1.1.1)
Description: This table contains general information about system phones.
systemPhoneTable
OID | Name | Type | Access
.1 | TerminalIndex | SystelTerminalIndex | RW
.2 | DeviceType | ENUM | RW
.3 | DevicePin | DisplayString | RW
.4 | ConfigDate | Date | R
.5 | ConfigSequenceNumber | INTEGER | R
.6 | OperStatus | ENUM | R
.7 | AdminStatus | ENUM | D
TerminalIndex
Reference to mpsTerminalTable, a unique value for each system phone. Range: 1 to 65535
DeviceType
Specified type of system phone. Enumerations: cs290 (20) cs410 (22) cs290u (23) cs410u (24) cs400 (25) ips290 (32) ips400 (33) ips290plus (34) s530 (64) s560 (65) ost-40 (144) ost-80 (145) ip120 (160) ip140 (161) dect150 (162) dect200-b (163) dect200-m (164) ip130 (165) de310-ip-pro (176) de410-ip-pro (177) de700-ip-pro (178) de900-ip-pro (179) n510-ip-pro (180) n720-ip-pro (181) n720-dm-pro (182)
DevicePin
The device PIN of the system phone (eg. to protect the configuration, settings or number programming menu of system phone). Length: 4 to 4
ConfigDate
The date of last configuration synchronization between PBX and system phone. Range: 0 to -1
ConfigSequenceNumber
A unique sequence number of the configuration data saved in the PBX and synchronized with the system phone. Range: 0 to 255
OperStatus
Operational state of the system phone. Enumerations: connected (1) unconnected (2) unsupported (3)
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH