>> MIB - Management Information Base
>> Table: certMgmtTable - (.1.3.6.1.4.1.272.4.26.33.7.1)
Description: This object specifies a task in the systems certMgmtTable. The system automatically deletes all tasks which have been finished except the most recent one.
certMgmtTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Command | ENUM | D
.3 | Url | DisplayString | RW
.4 | CertName | DisplayString | RW
.5 | SubjectName | DisplayString | RW
.6 | SubjectAltName | DisplayString | RW
.7 | SubjectAltName2 | DisplayString | RW
.8 | SubjectAltName3 | DisplayString | RW
.9 | KeyIndex | INTEGER | RW
.10 | CaCertIndex | INTEGER | RW
.11 | CaDomain | DisplayString | RW
.12 | Password | DisplayString | RW
.13 | AutoSave | ENUM | RW
.14 | PollInterval | INTEGER | RW
.15 | MaxPolls | INTEGER | RW
.16 | NumPolls | INTEGER | R
.17 | State | ENUM | R
.18 | RaSignCertIndex | INTEGER | RW
.19 | RaEncryptCertIndex | INTEGER | RW
.20 | KeyLength | INTEGER | RW
.21 | CaFingerprint | OCTET STRING | RW
.22 | NoCrls | ENUM | RW
Index
A unique index for this entry.
Command
The task to perform for this entry. Possible values: getca-scep(1), -- Retrieve CA certificate via SCEP enroll-scep(2), -- Enroll using SCEP enroll-manual(3), -- Do a manual enrollment delete(8) -- Cancel the task and delete this entry Enumerations: getca-scep (1) enroll-scep (2) enroll-manual (3) delete (8)
Url
The url to access for the task. Length: 0 to 255
CertName
The name of the resulting certificate (for certificate retrieval tasks) or the name of the certificate to use (for certificate export tasks. Length: 0 to 255
SubjectName
The subject name to include into the certificate request. Length: 0 to 255
SubjectAltName
The subject alternative name to include into the certificate request (optional). Length: 0 to 255
SubjectAltName2
A second subject alternative name (optional). Length: 0 to 255
SubjectAltName3
A third subject alternative name (optional). Length: 0 to 255
KeyIndex
The index of the key in the ipsecPublicKeyTable to use for certificate enrollment.
CaCertIndex
The index of the CA certificate to use (from the certTable).
CaDomain
The domain for which the CA certificate is to be received (getca_scep command only). Length: 0 to 255
Password
The password (SCEP: challenge password, CMP: <ref-no>:<psk>. Length: 0 to 255
AutoSave
Determines if pending requests should be saved permanently after each try and results should be saved permanently after finish. Enumerations: true (1) false (2)
PollInterval
The interval (in seconds) between polls. Range: 5 to 86400
MaxPolls
The maximum number of polls performed. A value of -1 means forever, a value of 0 disables polling, i.e. the task is cancelled if the initial result is delayed. Range: -1 to 32767
NumPolls
The number of polls already performed.
State
The state of the task specified by this entry. Enumerations: done (1) error (2) running (3) delayed (4) polling (5) notreached (6)
RaSignCertIndex
The index of the Registration Authority's (RA) certificate to use for signing purposes (from the certTable).
RaEncryptCertIndex
The index of the Registration Authority's (RA) certificate to use for encryption purposes (from the certTable).
KeyLength
The key length in bits used in requests for certificate enrollment.
CaFingerprint
This object holds the fingerprint of the CA certificate computed as an SHA1 or MD5 hash. This object is compared against an externally retrieved SHA1 / MD5 fingerprint (e.g. published on a CA's web site) to assure the authenticity of the certificate.
NoCrls
This object determines how CRL checking is set for certificates retrieved during certificate enrollment. Possible Values: true(1), -- do not check for certificate revocation -- lists for this CA (no meaning for non-CA -- certificates) false(2), -- check for certificate revocation -- lists for this CA (no meaning for non-CA -- certificates) auto(3), -- check for crls only if there is a -- CRLDistributionPoint in the certificate inherit(4), -- inherit from superior ca in chain. Enumerations: true (1) false (2) auto (3) inherit (4)

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH