>> MIB - Management Information Base
>> Table: qosIfTable - (.1.3.6.1.4.1.272.4.27.1.1)
Description: The qosIfTable enables QoS policies on the interface specified by qosIfIndex (interface index). Creating entries: Entries are created by assigning a value to the qosIfIndex object. Deleting entries: Entries are removed by setting an entry's qosIfType object to 'delete'.
qosIfTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | Type | ENUM | D
.3 | MaxTxRate | INTEGER | RW
.4 | TxRatePerVoipCall | INTEGER | RW
.6 | TxHeaderSize | INTEGER | RW
.7 | TxEncapOffset | INTEGER | RW
.8 | TxEncapMaxPadding | INTEGER | RW
Index
Unique interface index
Type
This object defines the queueing and scheduling algorithm used on the related interface, possible values: pq(1) = priority queueing wrr(2) = weighted round-robin scheduling wfq(3) = weighted fair queuing scheduling disable(8) = disable this entry delete(9) = delete this entry. Enumerations: pq (1) wrr (2) wfq (3) disabled (8) delete (9)
MaxTxRate
This object enables traffic shaping on the related interface, if set to zero (0) there is no shaping active. Otherwise this variable defines the maximum amount of bits per second to be transmitted.
TxRatePerVoipCall
Determines the amount of bandwidth (in bits per second) reserved dynamically by the QoS-scheduler for each accounted VoIP call (see qosIfStatCurrVoipCalls) in order to minimize latency / jitter for this type of data.
TxHeaderSize
Number of (lower layer protocol header) bytes per packet to be considered when calculating the bandwidth consumption. Range: 0 to 100
TxEncapOffset
Number of protocol header bytes per packet to be considered when calculating the bandwidth consumption. Range: 0 to 100
TxEncapMaxPadding
The maximum number of padding bytes per packet to be considered when calculating the bandwidth consumption. Note that the calcluation is done after adding qosIfTxEncapOffset bytes but before adding qosIfTxHeaderSize finally. Range: 0 to 100

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH