>> MIB - Management Information Base
>> Table: atmVpcTable - (.1.3.6.1.4.1.272.4.16.11.1)
Description: An entry in the table, containing information about a particular virtual path connection.
atmVpcTable
OID | Name | Type | Access
.1 | PortIndex | INTEGER | R
.2 | Vpi | INTEGER | R
.3 | OperStatus | ENUM | R
PortIndex
The interface index of the associated ATM hardware.
Vpi
The VPI value of this Virtual Path Connection. Range: 0 to 255
OperStatus
The present actual operational status of the VPC. A value of end2endUp(2) or end2endDown(3) would be used if the end-to-end status is known. If only local status information is available, a value of localUpEnd2endUnknown(4) or localDown(5) would be used. Enumerations: unknown (1) end2endUp (2) end2endDown (3) localUpEnd2endUnknown (4) localDown (5)

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH