>> MIB - Management Information Base
>> Table: ipTdrcServiceTable - (.1.3.6.1.4.1.272.4.5.44.1)
Description: The ipTdrcServiceTable specifies TCP services to be considered for the TCP Download Rate Control (TDRC) if enabled on the interface specified by ipTdrcServiceIfIndex (interface index). Creating entries: Entries are created by assigning an interface index to the ipTdrcServiceIfIndex object. Deleting entries: Entries are removed by setting an entry's ipTdrcServiceStatus object to 'delete'.
ipTdrcServiceTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | RW
.2 | Port | INTEGER | RW
.3 | Status | ENUM | D
.4 | Alias | DisplayString | RW
IfIndex
The associated Interface Index.
Port
The associated TCP service/port. Range: 0 to 65535
Status
The status of this entry. enabled(1): service will be TDRC controlled disabled(2): service will not be TDRC controlled delete(5): this entry will be deleted. Enumerations: enabled (1) disabled (2) delete (5)
Alias
Alias Name for the Service Entry Length: 0 to 255

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH