>> MIB - Management Information Base
>> Table: pimStarGITable - (.1.3.6.1.4.1.272.4.5.54.2.1.5.1)
Description: An entry (conceptual row) in the pimStarGITable.
pimStarGITable
OID | Name | Type | Access
.1 | IfIndex | InterfaceIndex | R
.2 | UpTime | TimeTicks | R
.3 | LocalMembership | ENUM | R
.4 | JoinPruneState | ENUM | R
.5 | PrunePendingTimer | TimeTicks | R
.6 | JoinExpiryTimer | TimeTicks | R
.7 | AssertState | ENUM | R
.8 | AssertTimer | TimeTicks | R
.9 | AssertWinnerAddressType | ENUM | R
.10 | AssertWinnerAddress | InetAddressIPv6 | R
.11 | AssertWinnerMetricPref | Unsigned32 | R
.12 | AssertWinnerMetric | Unsigned32 | R
IfIndex
The ifIndex of the interface that this entry corresponds to. Range: 1 to 2147483647
UpTime
The time since this entry was created by the local router.
LocalMembership
Whether the local router has (*,G) local membership on this interface (resulting from a mechanism such as IGMP or MLD). This corresponds to local_receiver_include(*,G,I) in the PIM-SM specification. Enumerations: true (1) false (2)
JoinPruneState
The state resulting from (*,G) Join/Prune messages received on this interface. This corresponds to the state of the downstream per-interface (*,G) state machine in the PIM-SM specification. Enumerations: noInfo (1) join (2) prunePending (3)
PrunePendingTimer
The time remaining before the local router acts on a (*,G) Prune message received on this interface, during which the router is waiting to see whether another downstream router will override the Prune message. This timer is called the (*,G) Prune-Pending Timer in the PIM-SM specification. This object is zero if the timer is not running.
JoinExpiryTimer
The time remaining before (*,G) Join state for this interface expires. This timer is called the (*,G) Join Expiry Timer in the PIM-SM specification. This object is zero if the timer is not running. A value of 'FFFFFFFF'h indicates an infinite expiry time.
AssertState
The (*,G) Assert state for this interface. This corresponds to the state of the per-interface (*,G) Assert state machine in the PIM-SM specification. If pimStarGPimMode is 'bidir', this object must be 'noInfo'. Enumerations: noInfo (1) iAmAssertWinner (2) iAmAssertLoser (3)
AssertTimer
If pimStarGIAssertState is 'iAmAssertWinner', this is the time remaining before the local router next sends a (*,G) Assert message on this interface. If pimStarGIAssertState is 'iAmAssertLoser', this is the time remaining before the (*,G) Assert state expires. If pimStarGIAssertState is 'noInfo', this is zero. This timer is called the (*,G) Assert Timer in the PIM-SM specification.
AssertWinnerAddressType
If pimStarGIAssertState is 'iAmAssertLoser', this is the address type of the assert winner; otherwise, this object is unknown(0). Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
AssertWinnerAddress
If pimStarGIAssertState is 'iAmAssertLoser', this is the address of the assert winner. The InetAddressType is given by the pimStarGIAssertWinnerAddressType object. Length: 16 to 16
AssertWinnerMetricPref
If pimStarGIAssertState is 'iAmAssertLoser', this is the metric preference of the route to the RP advertised by the assert winner; otherwise, this object is zero. Range: 0 to 2147483647
AssertWinnerMetric
If pimStarGIAssertState is 'iAmAssertLoser', this is the routing metric of the route to the RP advertised by the assert winner; otherwise, this object is zero.

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH