>> MIB - Management Information Base
>> Table: ipLfiTable - (.1.3.6.1.4.1.272.4.5.57.1)
Description: .
ipLfiTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | RW
.2 | Mode | ENUM | D
.10 | MaxFragSize | INTEGER | RW
.11 | MinFragSize | INTEGER | RW
.12 | CurrVoipCalls | INTEGER | RW
IfIndex
This object specifies the associated interface.
Mode
This object enables Link Framentation and Interleave (LFI) mode on the associated interface. Enumerations: enabled (1) disabled (2) delete (3) controlled-only (4) always (5)
MaxFragSize
This object specifies the current maximum fragment size used for Link Fragmentation and Interleave (LFI) mode on the associated interface.
MinFragSize
This object specifies the current minimum fragment size used for Link Fragmentation and Interleave (LFI) mode on the associated interface.
CurrVoipCalls
The current number of VoIP Calls routed via the associated interface. Range: 0 to 64

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH