>> MIB - Management Information Base
>> Table: imaGroupTable - (.1.3.6.1.4.1.272.4.54.1.1)
Description: An entry in the IMA Group table.
imaGroupTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.7 | Symmetry | ENUM | RC
.8 | MinNumTxLinks | INTEGER | RC
.9 | MinNumRxLinks | INTEGER | RC
.17 | TxFrameLength | ENUM | RC
.19 | DiffDelayMax | MilliSeconds | RC
.22 | AlphaValue | INTEGER | RC
.23 | BetaValue | INTEGER | RC
.24 | GammaValue | INTEGER | RC
.25 | ErrorsLinkDown | INTEGER | RC
.26 | ErrorIntervalLinkDown | INTEGER | RC
.27 | ErrorsLinkUp | INTEGER | RC
.28 | ErrorIntervalLinkUp | INTEGER | RC
.29 | MinLinkDownTime | INTEGER | RC
Index
A unique value for the IMA Group. Range: 1 to 2147483647
Symmetry
Symmetry of the IMA group. Enumerations: symmetricOperation (1) asymmetricOperation (2) asymmetricConfiguration (3)
MinNumTxLinks
Minimum number of transmit links required to be Active for the IMA group to be in the Operational state. Range: 1 to 32
MinNumRxLinks
Minimum number of receive links required to be Active for the IMA group to be in the Operational state. Range: 1 to 32
TxFrameLength
The frame length to be used by the IMA group in the transmit direction. Can only be set when the IMA group is startup. Enumerations: m32 (32) m64 (64) m128 (128) m256 (256)
DiffDelayMax
The maximum number of milliseconds of differential delay among the links that will be tolerated on this interface.
AlphaValue
This indicates the 'alpha' value used to specify the number of consecutive invalid ICP cells to be detected before moving to the IMA Hunt state from the IMA Sync state. Range: 1 to 2
BetaValue
This indicates the 'beta' value used to specify the number of consecutive errored ICP cells to be detected before moving to the IMA Hunt state from the IMA Sync state. Range: 1 to 5
GammaValue
This indicates the 'gamma' value used to specify the number of consecutive valid ICP cells to be detected before moving to the IMA Sync state from the IMA PreSync state. Range: 1 to 5
ErrorsLinkDown
This indicates the threshold of the number of ATM header errors per 100000 ATM cells, at which a link is inhibited. The number is compared with average value of received ATM header errors in the last time. The length of the considered time interval is configured in imaGroupErrorIntervalLinkDown. Range: 0 to 100000
ErrorIntervalLinkDown
This indicates the duration of the measure interval in seconds for the ATM header error counter. That is used for calculating an average, which is then compared with the imaGroupErrorsLinkDown value. Range: 15 to 3600
ErrorsLinkUp
This indicates the threshold of the number of ATM header errors per 100000 ATM cells, at which a link is enabled again. The number is compared with average value of received ATM header errors in the last time. The length of the considered time interval is configured in imaGroupErrorIntervalLinkUp. Range: 0 to 100000
ErrorIntervalLinkUp
This indicates the duration of the measure interval in seconds for the ATM header error counter. That is used for calculating an average, which is then compared with the imaGroupErrorsLinkUp value. Range: 15 to 3600
MinLinkDownTime
This indicates the minimum waiting time in seconds before a link can be enabled again, after it has been inhibited. Range: 0 to 3600

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH