>> MIB - Management Information Base
>> Table: sysInyRelais - (.1.3.6.1.4.1.272.4.17.5.1)
sysInyRelais
OID | Name | Type | Access
.1 | sysInyRelaisState | ENUM | RW
sysInyRelaisState
Relais control. off : Relais control coil is always off. on : Relais control coil is always on. alarm : Relais control coil controlled by failure LED. Enumerations: off (1) on (2) alarm (3)

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH