>> MIB - Management Information Base
>> Table: mpsTrunkGroupTable - (.1.3.6.1.4.1.272.4.53.3.3.1)
Description: This table contains global information about external trunk groups.
mpsTrunkGroupTable
OID | Name | Type | Access
.1 | Index | TrunkGroupIndex | RW
.2 | Layer2AlwaysOn | ENUM | RW
.3 | DefaultTargetType | ENUM | RW
.4 | DefaultTargetGroupIndex | GroupIndexOrZero | RW
.5 | DefaultTargetExtensionIndex | ExtensionIndexOrZero | RW
.6 | AdminStatus | ENUM | D
.7 | OutSigMode | ENUM | RW
.8 | BaseNumber | DisplayString | RW
.9 | FixedOutNumber | DisplayString | RW
.10 | DisplayName | DisplayString | RW
.11 | Facilities | BITS | RW
.12 | OutNumberType | ENUM | RW
.13 | InterfaceType | ENUM | RW
Index
A unique value for each trunk group. Range: 1 to 65535
Layer2AlwaysOn
This value determine if the Layer2 for this external isdn port is always on (1) or off (2). Enumerations: true (1) false (2)
DefaultTargetType
This variable contains the target type for misdialing, default is group. 'none' means no routing (busy signalling). 'global' -> use system target 'mpsSysConfigDefaultTargetType'. Enumerations: group (1) extension (2) global (3) none (4)
DefaultTargetGroupIndex
This variable contains the default target group index if the mpsTrunkGroupDefaultTargetType = group (1). Range: 0 to 99
DefaultTargetExtensionIndex
This variable contains the default target extension index if the mpsTrunkGroupDefaultTargetType = extension(2). Range: 0 to 65535
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
OutSigMode
This variable contains the outgoing signalling mode for this TrunkGroup. standard(1) : standard signalling cnsGlobal(2) : for all outgoing calls, the global CLIP no screening number will be used. cnsIndividual(3): for outgoing calls, individual settings can be used. fixedDDI(4) : for all outgoing calls, the mpsTrunkGroupBaseNumber + mpsTrunkGroupFixedOutNumber will be used. Enumerations: standard (1) cnsGlobal (2) cnsIndividual (3) fixedDDI (4)
BaseNumber
This variable contains the base number of the point-to-point port. Length: 0 to 20
FixedOutNumber
This variable contains the number for fixed outgoing number signalling. 1. mpsTrunkGroupOutSigMode = fixedDDI : the fixed DDI for outgoing calls. 2. mpsTrunkGroupOutSigMode = cnsGlobal: the global CLIP no screening number. Length: 0 to 20
DisplayName
Display name of the trunk group. Length: 0 to 32
Facilities
Special facilities for trunks. ignoreBaseNumber : for P-P-trunks - ignore base number for incoming calls. suppressBaseNumber: for P-P-trunks - don't send base number for outgoing calls. cnsSendRemoteCallerNumber: An incoming external call is forwarded to extern via 2nd b-channel to this trunk group, the original (extern) party was send as calling party number instead of the outgoing number for this trunk. suppressNotify: don't send HOLD/RETRIEVE notifications to ISDN trunk. Enumerations: ignoreBaseNumber (0) suppressBaseNumber (1) cnsSendRemoteCallerNumber (2) suppressNotify (3)
OutNumberType
This variable contains the type of number of the calling party for outgoing calls. 'default' means the type of number will be set by the PBX, otherwise use unknown, subscriber or national for fix setting. Enumerations: default (1) unknown (2) subscriber (3) national (4)
InterfaceType
This variable contains the interface type, for which type of interface this trunk group can be used. isdn-pmp(1) : isdn extern, point-to-multipoint isdn-pp(2) : isdn extern, point-to-point voip-pmp(3) : VoIP extern, point-to-multipoint voip-pp(4) : VoIP extern, point-to-point pots(5) : analoque extern, FXO Enumerations: isdn-pmp (1) isdn-pp (2) voip-pmp (3) voip-pp (4) pots (5)

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH