>> MIB - Management Information Base
>> Table: wlcVSSAuthProfileTable - (.1.3.6.1.4.1.272.4.61.1.31.1)
Description: This table contains the different VSS Authentication profiles.
wlcVSSAuthProfileTable
OID | Name | Type | Access
.1 | WlcVSSProfIndex | INTEGER | RC
.2 | ReAuthPeriod | INTEGER | RW
.3 | GroupRekeyStrict | ENUM | RW
.4 | GroupRekeyTime | INTEGER | RW
.5 | BlacklistTrials | INTEGER | RW
.6 | BlacklistTime | INTEGER | RW
.7 | BlacklistDuration | Unsigned32 | RW
WlcVSSProfIndex
Reference to VSS Profile entry (wlcVSSProfileIndex) this authentication parameters correspond to.
ReAuthPeriod
EAP reauthentication period in seconds (0=disabled). Range: 0 to 86400
GroupRekeyStrict
Rekey GTK when any STA that possesses the current GTK is leaving the BSS. Enumerations: true (1) false (2)
GroupRekeyTime
Time interval for rekeying GTK in seconds. Range: 1 to 604800
BlacklistTrials
The number of failed authentication trials per wlcVSSAuthProfileBlacklistTime before a station is stored into the dynamic blacklist.
BlacklistTime
The time within a station may perform wlcVSSAuthPRofileBlacklistTrials failed authentication trials, before it is temporatily blacklisted.
BlacklistDuration
The time a station is kept in the dynamic blacklist after too many failed authentication attempts. A value of 0 indicates forever.

MIB Reference to Software Version 9.1.7 generated on 2014/02/07. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH