>> MIB - Management Information Base
>> Table: voipSipAliasTable - (.1.3.6.1.4.1.272.4.33.6.16.1)
Description: Describes a call number translation entry.
voipSipAliasTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | Descr | DisplayString | RW
.3 | AdminStatus | ENUM | D
.4 | Local | DisplayString | RW
.5 | Remote | DisplayString | RW
.6 | Direction | ENUM | RW
.7 | Account | INTEGER | RW
Index
Unique index of entry.
Descr
User defined description of entry. Length: 0 to 30
AdminStatus
Administrative status of this call number translation entry: 'enable' -> The entry is enabled; 'disable' -> The entry is disabled. Default value is enable. Enumerations: enable (1) disable (2) delete (8)
Local
Local/internal number of an extension. Length: 0 to 30
Remote
External number of the same extension as referenced by 'Local'. Length: 0 to 30
Direction
Defines for which call directions this call number translation entry is checked: 'incoming' -> entry is checked only for incoming calls; 'outgoing' -> entry is checked only for outgoing calls; 'both' -> entry is always checked. Default value is both. Enumerations: incoming (1) outgoing (2) both (3)
Account
Table index number of an outgoing/incoming interface/account/line of a call (which triggers this call translation entry). That can be either a caller's ISDN or analog interface (on this gateway), a voipSipLineTable entry or a SIP provider account. For table index number ranges see 'SrcIf' of voipSipRouteTable.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH