>> MIB - Management Information Base
>> Table: serviceCallAdmin - (.1.3.6.1.4.1.272.4.22.8.1)
serviceCallAdmin
OID | Name | Type | Access
.1 | DaemonAdminStatus | ENUM | RW
.2 | DaemonOperStatus | ENUM | R
.3 | ServiceHostAddress | DisplayString | RW
.4 | ServiceHostPort | INTEGER | RW
.6 | DefaultShorthold | INTEGER | RW
DaemonAdminStatus
This object shows the current status of the service call daemon. It may be used to turn the service call daemon on and off. Enumerations: enabled (1) disabled (2)
DaemonOperStatus
This object shows the current operational state of the service call daemon. Enumerations: enabled (1) disabled (2)
ServiceHostAddress
This object identifies the host to be called on a service request. Length: 0 to 255
ServiceHostPort
This object identifies the port to be called on the service host.
DefaultShorthold
This object identifies the time in seconds to wait before closing an inactive service call.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH