>> MIB - Management Information Base
>> Table: serviceCallTable - (.1.3.6.1.4.1.272.4.22.8.2.1)
Description: An entry (conceptual row) representing a service call.
serviceCallTable
OID | Name | Type | Access
.1 | Index | INTEGER | RC
.2 | OperStatus | ENUM | R
.3 | AdminStatus | ENUM | D
.4 | Type | ENUM | RW
.5 | ForwardedService | ENUM | RW
.6 | ForwardedIP | IpAddress | RW
.7 | Ticket | DisplayString | RC
.8 | Duration | TimeTicks | R
Index
A unique identifier for a service call.
OperStatus
This object identifies the current operational state of this service call. Idle: The entry has been created but the daemon has not started calling yet. Start: The service call is started, but the authentication procedure is not yet done. Running: The service call is up and running. Done: The service call is completed and the row will be deleted. Error: Somewhere something went wrong. Blocked: Retry in a few seconds (This state usually is reached when network is currently unavailable. Enumerations: idle (1) start (2) running (3) done (4) error (5) blocked (6)
AdminStatus
This object identifies the current administrative state of this service call. Enumerations: enabled (1) disabled (2) delete (3)
Type
This object identifies the type of service call, it can either be the PBX itself or a phone attached to the pbx. Enumerations: pbx (1) phone (2)
ForwardedService
This object identifies the service to be forwarded to the service technician. The services are: Control: A commuication channel between serviced and B.A.B.E. used for signalling commands. Http: Http on port 80. Https: Https (using SSL) on port 443. Shell: Telnet using port 23. Trace: Bricktrace for packet capture analysis using port 7000. Enumerations: control (1) http (2) https (3) shell (4) trace (5)
ForwardedIP
This object identifies the IP address of the device the service call is pointed to.
Ticket
This object identifies the service ticket for this service call. Length: 0 to 14
Duration
This object identifies the duration of the current service call.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH