>> MIB - Management Information Base
>> Table: ikev2ProfileTable - (.1.3.6.1.4.1.272.4.26.22.1)
Description: This object contains an IKE_SA profile.
ikev2ProfileTable
OID | Name | Type | Access
.1 | Index | Unsigned32 | RW
.2 | Description | DisplayString | RW
.3 | Proposal | Unsigned32 | RW
.4 | BlockTime | INTEGER | RW
.5 | NatT | ENUM | D
.6 | MtuMax | INTEGER | RW
.7 | LifeSeconds | Unsigned32 | RW
.8 | AliveCheck | ENUM | RW
Index
A unique index identifying this entry. Range: 1 to -1
Description
An optional description for this profile. Length: 0 to 255
Proposal
The index of the first IKE proposal which may be used for IKE SA negotiation with this profile.
BlockTime
This object specifies the time in seconds for which a peer is blocked for any IPSec operations after a phase 1 initiator negotiation failed. Special values: -1: use settings from global profile (do not block by default) 0: do not block the peer at all. Range: -1 to 86400
NatT
This object specifies whether NAT-Traversal is enabled Possible values: enabled(1), -- enable Nat-Traversal disabled(2), -- disable Nat-Traversal default(3) -- use value from default profile -- (disabled, if this is the default profile). Enumerations: enabled (1) disabled (2) default (3) delete (4)
MtuMax
The maximum MTU value allowed for ipsecPeerMtu. Zero means use value from global profile, if this is the global profile, 1418 is assumed. Nonzero values smaller than 214 are reset to the minimum of 214. Range: 0 to 65535
LifeSeconds
The time (in seconds) after which an SA will be rekeyed.
AliveCheck
This object specifies if a check is done to see whether the other endpoint is alive. (only for IKEv2). Enumerations: enabled (1) disabled (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH