>> MIB - Management Information Base
>> Table: potsIfFxsTable - (.1.3.6.1.4.1.272.4.14.1.3.1)
Description: The potsIfFxsTable contains configuration information for the FXS outlets.
potsIfFxsTable
OID | Name | Type | Access
.1 | IfIndex | PotsIfIndex | RW
.2 | FlashMinTime | INTEGER | RW
.3 | FlashMaxTime | INTEGER | RW
.4 | RingLevel | INTEGER | RW
.5 | RingFreq | ENUM | RW
.6 | RingTableIndex | RingTabIndex | RW
.7 | ToneTableIndex | ToneTabIndex | RW
.8 | DataLinkType | BITS | RW
.9 | DataLinkElem | BITS | RW
.10 | DataLinkLevel | TransmitLevel | RW
.11 | DataLinkTiming | DataLinkTimerTabIndex | RW
.12 | DataLinkModeOnHook | ENUM | RW
.13 | DataLinkModeOffHook | ENUM | RW
.14 | DialPulseMinTimePulse | INTEGER | RW
.15 | DialPulseMaxTimePulse | INTEGER | RW
.16 | DialPulseMinTimePause | INTEGER | RW
.17 | DialPulseMaxTimePause | INTEGER | RW
IfIndex
Index of the FXS interface.
FlashMinTime
Minimum flash duration (ms). Flash pulses below this value will be ignored.
FlashMaxTime
Maximum flash duration (ms). Flash pulses above this value will be interpreted as hook-on.
RingLevel
Peak value of sinusoidal ringing voltage. Range: 0 to 150
RingFreq
Frequency of sinusoidal ringing voltage. Enumerations: freq25hz (1) freq50hz (2)
RingTableIndex
The ringing table index is the reference to all ringing cadences used for this extension. Definitions are in phoneIfRingTable.
ToneTableIndex
The tone table index refers to the tones used for this extension. Definitions are in phoneIfToneTable
DataLinkType
Allowed data transmission message types: setup - call setup message mwi - message waiting indicator message aoc - advice of charge message sms - short message service message Enumerations: setup (0) mwi (1) aoc (2) sms (3)
DataLinkElem
Allowed data transmission parameters (see ETSI EN 300 659-3). Not selected elements will be filtered out and not sent to the subscriber. Enumerations: date-time (0) calling-line-id (1) called-line-id (2) reason-for-absence-of-cli (3) calling-party-name (4) reason-for-absence-of-cpn (5) visual-indicator (6) message-identification (7) last-message-cli (8) complementary-date-time (9) complementary-cli (10) call-type (11) first-cli (12) no-of-messages (13) charge (14) additional-charge (15) duration-of-call (16) network-provider-id (17) carrier-id (18) select-terminal-function (19) display-information (20) service-information (21)
DataLinkLevel
Level of the data transmission signal (dB). Range: -30 to 0
DataLinkTiming
Index of the timer set to be used for on-hook and off-hook data transmission.
DataLinkModeOnHook
Selection of on-hook data transmission mode: 1: no on-hook data transmission 2: data transmission prior to ringing with DT-AS 3: data transmission prior to ringing with DT-AS and polarity reversal 4: data transmission prior to ringing with RP-AS 5: data transmission during ringing (after first ring) 6: data transmission using DTMF Enumerations: off (1) dt-as (2) dt-as-pol-rev (3) rp-as (4) during-ringing (5) dtmf (6)
DataLinkModeOffHook
Selection of off-hook data transmission mode: 1: no off-hook data transmission 2: data transmission prior using DT-AS Enumerations: off (1) dt-as (2)
DialPulseMinTimePulse
Pulse dialling break time minimum (ms). Break pulses below this limit will be ignored. Range: 10 to 100
DialPulseMaxTimePulse
Pulse dialling break time maximum (ms). A pause time above this limit is regarded as on-hook signal. Range: 50 to 200
DialPulseMinTimePause
Pulse dialling make time minimum (ms). Make pulses below this limit will be ignored. Range: 10 to 100
DialPulseMaxTimePause
Pulse dialling make time maximum (ms). A pause time above this limit finishes the pulse counting and this digit is regarded as complete. Range: 10 to 300

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH