>> MIB - Management Information Base
>> Table: mpsVoIPConfig - (.1.3.6.1.4.1.272.4.53.8.3)
mpsVoIPConfig
OID | Name | Type | Access
.1 | ConfigRtpPort | INTEGER | RW
.2 | RegTimer | Unsigned32 | RW
.3 | DscpSignalling | INTEGER | RW
.4 | ServerCertIndex | INTEGER | RW
.5 | SubscribeTimer | Unsigned32 | RW
ConfigRtpPort
Start value of dynamic RTP port.
RegTimer
Registration timer in seconds for IP extension. Set to 0 to get the time from the VoIP client.
DscpSignalling
The DSCP value used in IP header for signalling data. Range: 0 to 255
ServerCertIndex
Index of certificate entry in certTable to be used as server certificate for SIPS transport. If 0, predefined certificate of SIP stack is used.
SubscribeTimer
Timer value in seconds for SIP SUBSCRIBE session.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH