>> MIB - Management Information Base
>> Table: wlcLogHostProfileTable - (.1.3.6.1.4.1.272.4.61.1.11.1)
Description: The wlcLogHostProfileTable contains profiles to list hosts which are to receive syslog messages. This table also defines which types and levels of messages to send.
wlcLogHostProfileTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | AddrType | ENUM | RW
.3 | Addr | IpAddress | RW
.4 | Level | ENUM | D
.5 | Facility | ENUM | RW
.6 | Type | ENUM | RW
.7 | Timestamp | ENUM | RW
.8 | Method | ENUM | RW
Index
Unique index of a loghost profile
AddrType
The IP address type of the requested loghost. could be: -unknown(0): an unknown address type -ipv4(1) : an IPv4 address -ipv6(2) : an IPv6 address -ipv4z(3) : a non-global IPv4 address including a zone index -ipv6z(4) : a non-global IPv6 address including a zone index -dns(16) : a DNS domain name Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
Addr
IP Address where syslog messages are sent. If the facility is set to memory or console, this field is not used.
Level
Priorities lower than or equal to this level are sent to loghost. The delete priority is used to discard the whole entry. Enumerations: emerg (1) alert (2) crit (3) err (4) warning (5) notice (6) info (7) debug (8) delete (32)
Facility
The facility used for the syslog messages being generated. Enumerations: local0 (1) local1 (2) local2 (3) local3 (4) local4 (5) local5 (6) local6 (7) local7 (8)
Type
The subject of the messages that are to be generated. system means all subjects except accounting, all means all subjects. Enumerations: system (1) acct (2) all (3)
Timestamp
This object describes the format of the timestamp. none(1) = no timestamp, time(2) = only time is printed, all(3) = date and time is printed. Enumerations: none (1) time (2) all (3)
Method
This object provides protocol for sending syslog messages: udp(1) = udp tcp(2) = tcp Enumerations: udp (1) tcp (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH