>> MIB - Management Information Base
>> Table: ipDnsServerCfgTable - (.1.3.6.1.4.1.272.4.5.20.32.1)
Description: Contains manually configured nameserver-addresses and automatically added entries for DHCP/IPCP-assigned nameservers.
ipDnsServerCfgTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | Mode | ENUM | RW
.4 | Priority | INTEGER | RW
.5 | PrimaryAddress | IpAddress | RW
.6 | SecondaryAddress | IpAddress | RW
.7 | IfIndex | INTEGER | RW
.8 | Description | DisplayString | RW
.9 | Ip6PrimaryAddress | InetAddressIPv6 | RW
.10 | Ip6SecondaryAddress | InetAddressIPv6 | RW
Index
Unique index for unambiguous SNMP-addressing.
AdminStatus
Administrative status of this entry. Enumerations: enabled (1) disabled (2) delete (3)
Mode
Specifies whether nameserver-addresses are configured manually or updated automatically (see ipDnsDynamicGlobals) with each IPCP/DHCP-negotiation. Enumerations: manual (1) automatic (2)
Priority
Relative priority (0 is highest) of this entry. Range: 0 to 9
PrimaryAddress
IP-address of primary nameserver. Relevant only for manual entries (0 for automatic ones).
SecondaryAddress
IP-address of secondary nameserver. Relevant only for manual entries (0 for automatic ones).
IfIndex
Index of interface where nameservers are DHCP/IPCP-assigned. Relevant only for automatic entries (-1 for manual ones).
Description
Optional textual description for this nameserver-entry. Length: 0 to 64
Ip6PrimaryAddress
The primary DNS Server IPv6 Address.
Ip6SecondaryAddress
The secondary DNS Server IPv6 Address.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH