>> MIB - Management Information Base
>> Table: voipSipShortcutTable - (.1.3.6.1.4.1.272.4.33.6.17.1)
Description: Describes a shortcut (speed dial) entry.
voipSipShortcutTable
OID | Name | Type | Access
.1 | AdminStatus | ENUM | D
.2 | Descr | DisplayString | RW
.3 | Code | DisplayString | RW
.4 | Replace | DisplayString | RW
AdminStatus
The administration status of the shortcut entry: 'enable' -> the entry is active; 'disable' -> the entry is ignored; 'delete' -> delete the entry. Default value is enable. Enumerations: enable (1) disable (2) delete (8)
Descr
User defined description of entry. Length: 0 to 30
Code
Shortcut code. Note that no additional '*' is entered in this variable. The additional '*' a user has to dial in order to indicate a shortcut is automatically prefixed by the system. Length: 0 to 10
Replace
Replacement string for shortcut. May be any sequence of characters and numbers. Example: 'Code' is 30; 'Replace' is 003059876. So if you dial *30345 the dialed number is 003059876345. Length: 0 to 30

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH