>> MIB - Management Information Base
>> Table: dot11OperationTable - (.1.2.840.10036.2.1.1)
Description: An entry in the dot11OperationEntry Table. ifIndex - Each 802.11 interface is represented by an ifEntry. Interface tables in this MIB module are indexed by ifIndex.
dot11OperationTable
OID | Name | Type | Access
.1 | MACAddress | MacAddress | R
.2 | RTSThreshold | INTEGER | RW
.3 | ShortRetryLimit | INTEGER | RW
.4 | LongRetryLimit | INTEGER | RW
.5 | FragmentationThreshold | INTEGER | RW
.6 | MaxTransmitMSDULifetime | Unsigned32 | RW
.7 | MaxReceiveLifetime | Unsigned32 | RW
.8 | ManufacturerID | DisplayString | R
.9 | ProductID | DisplayString | R
.10 | CAPLimit | INTEGER | RW
.11 | HCCWmin | INTEGER | RW
.12 | HCCWmax | INTEGER | RW
.13 | HCCAIFSN | INTEGER | RW
.14 | ADDBAResponseTimeout | INTEGER | RW
.15 | ADDTSResponseTimeout | INTEGER | RW
.16 | ChannelUtilizationBeaconInterval | INTEGER | RW
.17 | ScheduleTimeout | INTEGER | RW
.18 | DLSResponseTimeout | INTEGER | RW
.19 | QAPMissingAckRetryLimit | INTEGER | RW
.20 | EDCAAveragingPeriod | INTEGER | RW
.21 | HTOperatingMode | ENUM | RW
.22 | RIFSMode | ENUM | RW
.23 | PSMPControlledAccess | ENUM | RW
.24 | ServiceIntervalGranularity | INTEGER | RW
.25 | DualCTSProtection | ENUM | RW
.26 | LSigTxopFullProtectionEnabled | ENUM | RW
.27 | NonGFEntitiesPresent | ENUM | RW
.28 | PCOActivated | ENUM | RW
.29 | PCO40MaxDuration | INTEGER | RW
.30 | PCO20MaxDuration | INTEGER | RW
.31 | PCO40MinDuration | INTEGER | RW
.32 | PCO20MinDuration | INTEGER | RW
MACAddress
Unique MAC Address assigned to the STA. Length: 6 to 6
RTSThreshold
This attribute shall indicate the number of octets in an PSDU, below which an RTS/CTS handshake shall not be performed, except as RTS/CTS is used as a cross modulation protection mechanism as defined in 9.10. An RTS/CTS handshake shall be performed at the beginning of any frame exchange sequence where the PSDU is of type Data or Management, the PSDU has an individual address in the Address1 field, and the length of the PSDU is greater than this threshold. (For additional details, refer to Table 21 in 9.7.) Setting this attribute to be larger than the maximum PSDU size shall have the effect of turning off the RTS/CTS handshake for frames of Data or Management type transmitted by this STA. Setting this attribute to zero shall have the effect of turning on the RTS/ CTS handshake for all frames of Data or Management type transmitted by this STA. The default value of this attribute shall be 65535. Range: 0 to 65535
ShortRetryLimit
This attribute shall indicate the maximum number of transmission attempts of a frame, the length of which is less than or equal to dot11RTSThreshold, that shall be made before a failure condition is indicated. The default value of this attribute shall be 7. Range: 1 to 255
LongRetryLimit
This attribute shall indicate the maximum number of transmission attempts of a frame, the length of which is greater than dot11RTSThreshold, that shall be made before a failure condition is indicated. The default value of this attribute shall be 4. Range: 1 to 255
FragmentationThreshold
This attribute shall specify the current maximum size, in octets, of the PSDU that may be delivered to the PHY. This maximum size does not apply in the case of A-MPDU. An MSDU, A-MSDU or MMPDU shall be broken into fragments if its size exceeds the value of this attribute after adding MAC headers and trailers. An MSDU, A-MSDU or MMPDU shall be fragmented when the resulting frame has an individual address in the Address1 field, and the length of the frame is larger than this threshold. The default value for this attribute shall be the lesser of 8000 or the aMPDUMaxLength or the aPSDUMaxLength of the attached PHY and shall never exceed the lesser of 8000 or the aMPDUMaxLength or the aPSDUMaxLength of the attached PHY. The value of this attribute shall never be less than 256. Range: 256 to 8000
MaxTransmitMSDULifetime
The MaxTransmitMSDULifetime shall be the elapsed time in TU, after the initial transmission of an MSDU, after which further attempts to transmit the MSDU shall be terminated. The default value of this attribute shall be 512. Range: 1 to -1
MaxReceiveLifetime
The MaxReceiveLifetime shall be the elapsed time in TU, after the initial reception of a fragmented MMPDU or MSDU, after which further attempts to reassemble the MMPDU or MSDU shall be terminated. The default value shall be 512. Range: 1 to -1
ManufacturerID
The ManufacturerID shall include, at a minimum, the name of the manufacturer. It may include additional information at the manufacturer's discretion. The default value of this attribute shall be null. Length: 0 to 128
ProductID
The ProductID shall include, at a minimum, an identifier that is unique to the manufacturer. It may include additional information at the manufacturer's discretion. The default value of this attribute shall be null. Length: 0 to 128
CAPLimit
This attribute shall specify the maximum number of TUs a Controlled access phase(CAP) can last.
HCCWmin
This attribute shall specify the value of the minimum size of the window that shall be used by the HC for generating a random number for the backoff. The value of this attribute shall be such that it could always be expressed in the form of 2X - 1, where X is an integer. The default value of this attribute shall be 0. Range: 0 to 255
HCCWmax
This attribute shall specify the value of the maximum size of the window that shall be used by the HC for generating a random number for the backoff. The value of this attribute shall be such that it could always be expressed in the form of 2X - 1, where X is an integer. The default value of this attribute shall be 0. Range: 0 to 255
HCCAIFSN
This attribute shall specify the number of slots, after a SIFS duration, that the HC shall sense the medium idle either before transmitting or executing a backoff. The default value of this attribute shall be 1. Range: 1 to 15
ADDBAResponseTimeout
This attribute shall specify the maximum number of seconds a BA is to be responded. The default value of this attribute shall be 1. Range: 1 to 65535
ADDTSResponseTimeout
This attribute shall specify the maximum number of seconds an ADDTS request is to be responded. The default value of this attribute shall be 1. Range: 1 to 65535
ChannelUtilizationBeaconInterval
This attribute shall indicate the number of beacon intervals over which the channel busy time should be averaged. The default value for this parameter shall be 50. Range: 1 to 100
ScheduleTimeout
This attribute shall indicate the duration in TUs after which a STA could go into power-save mode. The default value for this parameter shall be 10. Range: 1 to 100
DLSResponseTimeout
This attribute shall specify the maximum number of seconds a direct link request is to be responded. The default value of this attribute shall be 10. Range: 1 to 65535
QAPMissingAckRetryLimit
This attribute indicates the number of times the QAP may retry a frame for which it does not receive an ACK for a STA in power-save mode after receiving a PS-Poll and sending a directed response or after the QAP does not receive an ACK to a directed MPDU sent with the EOSP set to 1. Range: 1 to 100
EDCAAveragingPeriod
This attribute shall indicate the number of seconds over which the admitted_time and used_time are computed. The default value for this parameter shall be 5. Range: 1 to 100
HTOperatingMode
This attribute indicates the level of protection that needs to be provided to the transmissions in an IEEE 802.11 network with HT STAs. The default value of this attribute is 0. Enumerations: htPure (0) optionalProtection (1) mandatoryFortyProtection (2) mandatoryAllProtection (3)
RIFSMode
This attribute, when TRUE, indicates that RIFS mode is allowed in the BSS. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
PSMPControlledAccess
This attribute, when TRUE indicates that the AP accepts associations only from stations for which dot11PSMPOptionImplemented is TRUE. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
ServiceIntervalGranularity
This attribute indicates the Service Interval Granularity to be used for scheduled PSMP. The value of the granularity is given by (dot11ServiceIntervalGranularity+1)*5 milliseconds. The default value of this attribute is 0. Range: 0 to 7
DualCTSProtection
This attribute, when TRUE indicates that the AP uses dual CTS protection to protect the non-STBC frame and STBC frame transmissions. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
LSigTxopFullProtectionEnabled
This attribute, when TRUE, indicates that the LSIG TXOP Protection may be used by stations that have the attribute dot11LSigTxopProtectionOptionImplemented set to TRUE. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
NonGFEntitiesPresent
This attribute, when TRUE, indicates that STA that are not Greenfield Capable are present in the BSS. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
PCOActivated
This attribute, when TRUE, indicates that the PCO is activated. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
PCO40MaxDuration
The attribute indicates the maximum duration of 40 MHz phase in TU under PCO operation. The default value of this attribute shall be 60. The value of this attribute shall be equal to or larger than dot11PCO40MinDuration. Range: 1 to 65535
PCO20MaxDuration
The attribute indicates the maximum duration of 20 MHz phase in TU under PCO operation. The default value of this attribute shall be 60. The value of this attribute shall be equal to or larger than dot11PCO20MinDuration. Range: 1 to 65535
PCO40MinDuration
The attribute indicates the minimum duration of 40 MHz phase in TU under PCO operation. The default value of this attribute shall be 40. Range: 1 to 65535
PCO20MinDuration
The attribute indicates the minimum duration of 20 MHz phase in TU under PCO operation. The default value of this attribute shall be 40. Range: 1 to 65535

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH