>> MIB - Management Information Base
>> Table: ipAddrTable - (.1.3.6.1.2.1.4.20.1)
Description: The addressing information for one of this entity's IP addresses.
ipAddrTable
OID | Name | Type | Access
.1 | Addr | IpAddress | R
.2 | IfIndex | INTEGER | R
.3 | NetMask | IpAddress | R
.4 | BcastAddr | INTEGER | R
.5 | ReasmMaxSize | INTEGER | R
Addr
The IP address to which this entry's addressing information pertains.
IfIndex
The index value which uniquely identifies the interface to which this entry is applicable. The interface identified by a particular value of this index is the same interface as identified by the same value of RFC 1573's ifIndex. Range: 1 to 2147483647
NetMask
The subnet mask associated with the IP address of this entry. The value of the mask is an IP address with all the network bits set to 1 and all the hosts bits set to 0.
BcastAddr
The value of the least-significant bit in the IP broadcast address used for sending datagrams on the (logical) interface associated with the IP address of this entry. For example, when the Internet standard all-ones broadcast address is used, the value will be 1. This value applies to both the subnet and network broadcasts addresses used by the entity on this (logical) interface. Range: 0 to 1
ReasmMaxSize
The size of the largest IP datagram which this entity can re-assemble from incoming IP fragmented datagrams received on this interface. Range: 0 to 65535

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH