>> MIB - Management Information Base
>> Table: dot11RSNAStatsTable - (.1.2.840.10036.1.12.1)
Description: An entry in the dot11RSNAStatsTable.
dot11RSNAStatsTable
OID | Name | Type | Access
.1 | Index | Unsigned32 | R
.2 | STAAddress | MacAddress | R
.3 | Version | Unsigned32 | R
.4 | SelectedPairwiseCipher | OCTET STRING | R
.5 | TKIPICVErrors | Counter32 | R
.6 | TKIPLocalMICFailures | Counter32 | R
.7 | TKIPRemoteMICFailures | Counter32 | R
.8 | CCMPReplays | Counter32 | R
.9 | CCMPDecryptErrors | Counter32 | R
.10 | TKIPReplays | Counter32 | R
Index
An auxiliary index into the dot11RSNAStatsTable. Range: 1 to -1
STAAddress
The MAC address of the STA to which the statistics in this conceptual row belong. Length: 6 to 6
Version
The RSNA version with which the STA associated. Range: 1 to -1
SelectedPairwiseCipher
The pairwise cipher suite Selector (as defined in 7.3.29.1) used during association, in transmission order. Length: 4 to 4
TKIPICVErrors
Counts the number of TKIP ICV errors encountered when decrypting packets for the STA.
TKIPLocalMICFailures
Counts the number of MIC failures encountered when checking the integrity of packets received from the STA at this entity.
TKIPRemoteMICFailures
Counts the number of MIC failures encountered by the STA identified by dot11StatsSTAAddress and reported back to this entity.
CCMPReplays
The number of received CCMP MPDUs discarded by the replay mechanism.
CCMPDecryptErrors
The number of received MPDUs discarded by the CCMP decryption algorithm.
TKIPReplays
Counts the number of TKIP replay errors detected.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH