>> MIB - Management Information Base
>> Table: dot1dTpPortTable - (.1.3.6.1.4.1.272.4.8.4.4.1)
Description: A list of information for each port of a transparent bridge.
dot1dTpPortTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | MaxInfo | INTEGER | R
.3 | InFrames | Counter | R
.4 | OutFrames | Counter | R
.5 | InDiscards | Counter | R
IfIndex
The port number of the port for which this entry contains Transparent bridging management information.
MaxInfo
The maximum size of the INFO (non-MAC) field that this port will receive or transmit.
InFrames
The number of frames that have been received by this port from its segment. Note that a frame received on the interface corresponding to this port is only counted by this object if and only if it is for a protocol being processed by the local bridging function, including bridge management frames.
OutFrames
The number of frames that have been transmitted by this port to its segment. Note that a frame transmitted on the interface corresponding to this port is only counted by this object if and only if it is for a protocol being processed by the local bridging function, including bridge management frames.
InDiscards
Count of valid frames received which were discarded (i.e., filtered) by the forwarding process.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH