>> MIB - Management Information Base
>> Table: l2tpSessionTable - (.1.3.6.1.4.1.272.4.23.8.40.10)
Description: Entries in this table are created by the system.
l2tpSessionTable
OID | Name | Type | Access
.10 | RemoteIpAddress | IpAddress | R
.20 | RemoteUdpPort | INTEGER | R
.30 | RemoteTunnelId | INTEGER | R
.40 | RemoteSessionId | INTEGER | R
.50 | RemoteHostname | DisplayString | R
.60 | LocalIpAddress | IpAddress | R
.70 | LocalUdpPort | INTEGER | R
.80 | LocalTunnelId | INTEGER | R
.90 | LocalSessionId | INTEGER | R
.100 | LocalHostname | DisplayString | R
.110 | CallSerialNumber | INTEGER | R
.120 | DataSequencing | ENUM | RW
.130 | State | ENUM | RW
.140 | Info | DisplayString | R
.150 | ClientPPPCrcErrors | INTEGER | R
.160 | ClientPPPFramingErrors | INTEGER | R
.170 | ClientPPPHardwareOverruns | INTEGER | R
.180 | ClientPPPBufferOverruns | INTEGER | R
.190 | ClientPPPTimeoutErrors | INTEGER | R
.200 | ClientPPPAlignmentErrors | INTEGER | R
RemoteIpAddress
The remote IP address for the tunnel.
RemoteUdpPort
The remote UDP port number for the tunnel. Range: 0 to 65535
RemoteTunnelId
The ID used by the remote end for the tunnel. Range: 0 to 65535
RemoteSessionId
The ID used by the remote end for the session. Range: 0 to 65535
RemoteHostname
The name of the remote host. Length: 0 to 255
LocalIpAddress
The local IP address for the tunnel.
LocalUdpPort
The local UDP port number for the tunnel. Range: 0 to 65535
LocalTunnelId
The ID used by the local end for the tunnel. Range: 0 to 65535
LocalSessionId
The ID used by the local end for the session. Range: 0 to 65535
LocalHostname
The name of the local host. Length: 0 to 255
CallSerialNumber
The call serial number for the session.
DataSequencing
This object specifies if sequence numbers are used on the data channel of the session. Enumerations: disabled (2) enabled (3)
State
The current state of the session as specified in RFC2661. Selecting shutdown(7) value results in session hangup. Any other value is ignored. Enumerations: idle (1) waittunnel (2) waitcsanswer (3) waitreply (4) waitconnect (5) established (6) shutdown (7)
Info
Info on the state of the session. Length: 0 to 255
ClientPPPCrcErrors
The number of PPP CRC errors detected by the LAC while communicating with the PPP client. This value is only significant in L2TP-LNS mode.
ClientPPPFramingErrors
The number of PPP framing errors detected by the LAC while communicating with the PPP client. This value is only significant in L2TP-LNS mode.
ClientPPPHardwareOverruns
The number of PPP hardware overruns detected by the LAC while communicating with the PPP client. This value is only significant in L2TP-LNS mode.
ClientPPPBufferOverruns
The number of PPP buffer overruns detected by the LAC while communicating with the PPP client. This value is only significant in L2TP-LNS mode.
ClientPPPTimeoutErrors
The number of PPP timeout errors detected by the LAC while communicating with the PPP client. This value is only significant in L2TP-LNS mode.
ClientPPPAlignmentErrors
The number of PPP alignment errors detected by the LAC while communicating with the PPP client. This value is only significant in L2TP-LNS mode.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH