>> MIB - Management Information Base
>> Table: adslAturPhysTable - (.1.3.6.1.4.1.272.4.30.1.1.3.1)
Description: An entry in the adslAturPhysTable.
adslAturPhysTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | InvSerialNumber | DisplayString | R
.3 | InvVendorID | DisplayString | R
.4 | InvVersionNumber | DisplayString | R
.5 | CurrSnrMgn | INTEGER | R
.6 | CurrAtn | INTEGER | R
.7 | CurrStatus | ENUM | R
.8 | CurrOutputPwr | INTEGER | R
.9 | CurrAttainableRate | INTEGER | RW
.10 | CurrPowercutback | INTEGER | R
IfIndex
Specifies the ADSL interface index.
InvSerialNumber
The vendor specific string that identifies the vendor equipment. Length: 0 to 32
InvVendorID
The vendor ID code is a copy of the binary vendor identification field defined by the PHY[10] and expressed as readable characters. Length: 0 to 16
InvVersionNumber
The vendor specific version number sent by this ATU as part of the initialization messages. It is a copy of the binary version number field defined by the PHY[10] and expressed as readable characters. Length: 0 to 16
CurrSnrMgn
Noise Margin as seen by this ATU with respect to its received signal in tenth dB. Range: -640 to 640
CurrAtn
Measured difference between the total power transmitted by the peer ATU and the total power received by this ATU in tenth dB. Range: 0 to 630
CurrStatus
Indicates mandatory state of the ATUR line, i.e. the state of the line as seen by ATUR. This is a bit-map of possible conditions. Due to the isolation of the ATUR when line problems occur, many state conditions like loss of power, loss of quality signal, and initialization errors, can not be determined. While trouble shooting ATUR, also use object, adslAtucCurrStatus. The various bit positions are: 1 noDefect There no defects on the line 2 lossOfFraming ATUR failure due to not receiving valid frame 3 lossOfSignal ATUR failure due to not receiving signal 4 lossOfPower ATUR failure due to loss of power 5 lossOfSignalQuality Loss of Signal Quality is declared when the Noise Margin falls below the Minimum Noise Margin, or the bit-error-rate exceeds 10^-7. 6 lossOfCellDelineation ATUR failure due loss of Cell Delineation in interleaved and non-interleaved mode. This is intended to supplement ifOperStatus. Enumerations: noDefect (1) lossOfFraming (2) lossOfSignal (3) lossOfPower (4) lossOfSignalQuality (5) lossOfCellDelineation (6)
CurrOutputPwr
Measured total output power transmitted by this ATU. This is the measurement that was reported during the last activation sequence in tenth dB. Range: -310 to 310
CurrAttainableRate
Indicates the maximum mandatoryly attainable data rate by the ATU. This value will be equal or greater than the mandatory line rate. Range: 32000 to 2560000
CurrPowercutback
Indicates the powercutback by the ATU in tenth dB.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH