>> MIB - Management Information Base
>> Table: udpTable - (.1.3.6.1.2.1.7.5.1)
Description: Information about a particular current UDP listener.
udpTable
OID | Name | Type | Access
.1 | Address | IpAddress | R
.2 | Port | INTEGER | R
Address
The local IP address for this UDP listener. In the case of a UDP listener which is willing to accept datagrams for any IP interface associated with the node, the value 0.0.0.0 is used.
Port
The local port number for this UDP listener. Range: 0 to 65535

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH