>> MIB - Management Information Base
>> Table: pppoePassThroughTable - (.1.3.6.1.4.1.272.4.24.5.1)
Description: The pppoePassThroughTable is used to enable the PPPoE mode between the two specified Ethernet interfaces. Creating entries: Entries are added by the user. Deleting entries: Entries are removed once the respective variable pppoePassThroughStatus is set to delete(3).
pppoePassThroughTable
OID | Name | Type | Access
.1 | EthIfIndex1 | INTEGER | RW
.2 | EthIfIndex2 | INTEGER | RW
.3 | Status | ENUM | D
EthIfIndex1
The interface index (ifIndex) of the first associated Ethernet interface.
EthIfIndex2
The interface index (ifIndex) of the secondassociated Ethernet interface.
Status
The administrative status of this entry. Enumerations: enabled (1) disabled (2) delete (3)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH