>> MIB - Management Information Base
>> Table: qosTosStatTable - (.1.3.6.1.4.1.272.4.27.5.1)
Description: The qosTosStatTable contains statistical QoS-specific information by qosTosStatTos (index) for each interface specified by qosTosStatIfIndex (interface index). Only the system can add or delete entries to this table.
qosTosStatTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Tos | INTEGER | R
.3 | OutPkts | Counter32 | R
.5 | InPkts | Counter32 | R
.7 | PktsDropped | Counter32 | R
.9 | State | ENUM | RW
.10 | HCOutOctets | Counter64 | R
.11 | HCInOctets | Counter64 | R
.12 | HCOctetsDropped | Counter64 | R
IfIndex
The unique interface index for which statistics are managed.
Tos
The TOS value for which statistics are managed. Range: 0 to 255
OutPkts
The number of packets sent with a TOS set to qosTosStatTos on the qosTosStatIfIndex interface.
InPkts
The number of packets received with a TOS set to qosTosStatTos on the qosTosStatIfIndex interface.
PktsDropped
The number of outgoing packets dropped with a TOS set to qosTosStatTos on the qosTosStatIfIndex interface.
State
This object allows statistics to be reinitialized. Possible values: running(1) = no reset of statistics reset(2) = reset all counters in this entry. When the reset action is over, this object is automatically restored to its 'running(1)' default state. Enumerations: running (1) reset (2)
HCOutOctets
The number of octets sent in packets with a TOS set to qosTosStatTos on the qosTosStatIfIndex interface.
HCInOctets
The number of octets received in packets with a TOS set to qosTosStatTos on the qosTosStatIfIndex interface.
HCOctetsDropped
The number of octets in outgoing packets dropped with a TOS set to qosTosStatTos on the qosTosStatIfIndex interface.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH