>> MIB - Management Information Base
>> Table: ospfAreaTable - (.1.3.6.1.2.1.14.2.1)
Description: Information describing the configured parameters and cumulative statistics of one of the router's attached areas.
ospfAreaTable
OID | Name | Type | Access
.1 | AreaId | IpAddress | RW
.2 | AuthType | INTEGER | R
.3 | ImportAsExtern | ENUM | RW
.4 | SpfRuns | Counter | R
.5 | AreaBdrRtrCount | Gauge | R
.6 | AsBdrRtrCount | Gauge | R
.7 | AreaLsaCount | Gauge | R
.8 | AreaLsaCksumSum | HexValue | R
.9 | AreaSummary | ENUM | RW
.10 | AreaStatus | ENUM | D
.11 | AreaLSAOriginateDelay | INTEGER | RW
AreaId
A 32-bit integer uniquely identifying an area. Area ID 0.0.0.0 is used for the OSPF backbone.
AuthType
The authentication type specified for an area. Additional authentication types may be assigned locally on a per Area basis. ** not used - see ospfIfAuthType ** Range: 0 to 255
ImportAsExtern
The area's support for importing AS external link- state advertisements. Enumerations: importExternal (1) importNoExternal (2) importNssa (3)
SpfRuns
The number of times that the intra-area route table has been calculated using this area's link-state database. This is typically done using Dijkstra's algorithm.
AreaBdrRtrCount
The total number of area border routers reachable within this area. This is initially zero, and is calculated in each SPF Pass.
AsBdrRtrCount
The total number of Autonomous System border routers reachable within this area. This is initially zero, and is calculated in each SPF Pass.
AreaLsaCount
The total number of link-state advertisements in this area's link-state database, excluding AS External LSA's.
AreaLsaCksumSum
The 32-bit unsigned sum of the link-state advertisements' LS checksums contained in this area's link-state database. This sum excludes external (LS type 5) link-state advertisements. The sum can be used to determine if there has been a change in a router's link state database, and to compare the link-state database of two routers. Range: 0 to -1
AreaSummary
The variable ospfAreaSummary controls the im- port of summary LSAs into stub areas. It has no effect on other areas. If it is noAreaSummary, the router will neither originate nor propagate summary LSAs into the stub area. It will rely entirely on its de- fault route. If it is sendAreaSummary, the router will both summarize and propagate summary LSAs. Enumerations: noAreaSummary (1) sendAreaSummary (2)
AreaStatus
This variable displays the status of the en- try. Setting it to 'invalid' has the effect of rendering it inoperative. The internal effect (row removal) is implementation dependent. Enumerations: valid (1) invalid (2)
AreaLSAOriginateDelay
The variable ospfAreaLSAOriginateDelay controls the origination of LSA for RADIUS-DialUp connections. It has no effect on other areas. The unit of the value of this variable is 1/100 seconds, the range lies between 0 and 500 miliseconds and the default value is 0. If it is greater then 0, then the origination of LSA will be delayed for this time. This period of time is necessary, when the RADIUS-Dialup connection generates more then one (Host-)Route. Range: 0 to 500

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH