>> MIB - Management Information Base
>> Table: mobileSimCfgTable - (.1.3.6.1.4.1.272.4.41.4.1.21.1)
Description: A single mobileSimCfgTable entry.
mobileSimCfgTable
OID | Name | Type | Access
.1 | IccId | DisplayString | RW
.2 | PIN | DisplayString | RW
.3 | PUK | DisplayString | RW
.4 | APN | DisplayString | RW
.5 | AccessMode | ENUM | D
.6 | RoamingMode | ENUM | RW
.7 | RoamingPLMN | INTEGER | RW
.8 | Dispatch | ENUM | RW
.9 | GsmFallback | DisplayString | RW
.15 | CugAddr | IpAddress | RW
.16 | CugAuth | ENUM | RW
.17 | CugUser | DisplayString | RW
.18 | CugPwd | DisplayString | RW
.19 | OperatorScan | ENUM | RW
.20 | PinData | OCTET STRING | N
.21 | CugAPN | DisplayString | RW
IccId
The ICC-ID of the used SIM-Card to configure. Unfortunately some UMTS modem vendors offer no capability to read this ID before entering the valid PIN :-( Length: 0 to 32
PIN
The PIN code of the SIM card. This is used to authorize the access to the SIM-Card. Length: 0 to 8
PUK
The PUK code of the SIM card. Needed in case of wrong PIN input for three times in a row. Length: 0 to 16
APN
GPRS APN (Access Point Name) used by this SIM-Card. Length: 0 to 80
AccessMode
The default Access Type to be used by the GPRS/UMTS/LTE Modem. This setting depends on local network availability and therefore it's bound to the network operator specific SIM-Card. Possible settings are: auto(1) -- factory default settings gprs-only(2) -- GPRS only (no UMTS/LTE) umts-only(3) -- UMTS only (no GPRS/LTE) gprs-pref(4) -- GPRS preferred (Priority 2G/3G/xxx) umts-pref(5) -- UMTS preferred (Priority 3G/2G/xxx) lte-only(7) -- LTE only lte-pref(8) -- LTE preferred (Priority 4G/3G/2G) lte-umts(9) -- Priority 4G/3G, no GPRS lte-gprs(10) -- Priority 4G/2G, no UMTS lte-gprs-umts(11) -- Priority 4G/2G/3G umts-lte(12) -- Priority 3G/4G, no GPRS umts-gprs(13) -- Priority 3G/2G, no LTE umts-lte-gprs(14) -- Priority 3G/4G/2G gprs-lte(15) -- Priority 2G/4G, no UMTS gprs-umts(16) -- Priority 2G/3G, no LTE gprs-lte-umts(17) -- Priority 2G/4G/3G Not all possible settings make sense and/or are supported by all LTE capable Modems. Enumerations: auto (1) gprs-only (2) umts-only (3) gprs-pref (4) umts-pref (5) delete (6) lte-only (7) lte-pref (8) lte-umts (9) lte-gprs (10) lte-gprs-umts (11) umts-lte (12) umts-gprs (13) umts-lte-gprs (14) gprs-lte (15) gprs-umts (16) gprs-lte-umts (17)
RoamingMode
The Roaming configuration for this mobile interface. Possible values are: disabled - no roaming at all auto - roaming decision by modems factory defaults unrestricted - no restrictions for roaming decision international - international roaming only national - national roaming only fixed - use mobileConfigRoamingPLMN exclusively full-auto - let the modem select the roaming partner Enumerations: disabled (1) auto (2) unrestricted (3) international (4) national (5) fixed (6) full-auto (7)
RoamingPLMN
The PLMN (Public Land Mobile Netword) code used for Roaming. Used only if mobileDevCfgRoamingMode_fixed is selected.
Dispatch
The dispatch service the Modem should be used for. The SIM-Card should support/enable basic functionality to use the service (eg access circuit switched networks to use V.110 and/or V.120). Routing tasks (IP, IPX, X.25, bridging, ...) should use ppp(1). For isdnlogin program use the isdnlogin(2) item. For IPSec callback use item ipsec(60). Enumerations: ppp (1) isdnlogin (2) none (3) ppp-modem (13) ppp-v110-1200 (15) ppp-v110-2400 (16) ppp-v110-4800 (17) ppp-v110-9600 (18) ppp-v110-14400 (19) ppp-v110-19200 (20) ppp-v110-38400 (21) ppp-v120 (23) ppp-modem-profile-1 (26) ppp-modem-profile-2 (27) ppp-modem-profile-3 (28) ppp-modem-profile-4 (29) ppp-modem-profile-5 (30) ppp-modem-profile-6 (31) ppp-modem-profile-7 (32) ppp-modem-profile-8 (33) ipsec (60)
GsmFallback
If the Router is called using the GsmFallback number the actual connection is dropped and the Access Type is switched back from UMTS to GSM. Length: 0 to 32
CugAddr
The provider assigned IP-Address if any.
CugAuth
The authentication method to be used. Enumerations: none (1) pap (2) chap (3) pap-chap (4)
CugUser
The provider assigned user name. Length: 0 to 255
CugPwd
The provider assigned password. Length: 0 to 255
OperatorScan
Handling of scanning available Providers (PLMN) never - use only home or fixed PLMN startup - scan on startup, only for information always - used for using roaming PLMN outside own country Enumerations: never (1) startup (2) always (3)
PinData
Not accessible entry for storing the PIN permanently. This is a security feature (?) used by France Telecom. Length: 0 to 16
CugAPN
Closed User Group authentication APN, may be different from registration APN. Length: 0 to 80

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH