>> MIB - Management Information Base
>> Table: igmpAdmin - (.1.3.6.1.4.1.272.4.5.51.1)
igmpAdmin
OID | Name | Type | Access
.1 | Status | ENUM | RW
.2 | Mode | ENUM | RW
.3 | MaxGroups | INTEGER | RW
.4 | MaxSources | INTEGER | RW
.5 | StateLimit | INTEGER | RW
.6 | Logging | ENUM | RW
Status
This object shows the current status of IGMP. It may be used to turn on or off IGMP. If set to auto IGMP will create host-only interfaces automatically as soon as applications request it. Enumerations: up (1) down (2) auto (3)
Mode
This object show the current operation mode of IGMP. With compat IGMP runs in compatibility mode, accepting IGMP v1,v2,v3 packets. Running in v3only mode, only IGMP v3 packets are accepted. Enumerations: compat (1) v3only (2)
MaxGroups
This object specifies the maximum number of groups. Range: 1 to 65535
MaxSources
This object specifies the maximum number of sources. Range: 1 to 65535
StateLimit
The maximum allowed number of Reports/Queries per seconds globally on a router. Must be greater zero to be active. Range: 0 to 65535
Logging
This object might be used to define the behaviour of generated syslog messages: off - be quiet normal - critical error messages are generated verbose - creates messages about what IGMP is currently doing Enumerations: off (0) normal (1) verbose (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH