>> MIB - Management Information Base
>> Table: hdsl2ShdslInventoryTable - (.1.3.6.1.4.1.272.4.35.1.1.3.1)
Description: An entry in the hdsl2ShdslInventoryTable. Each entry represents inventory information for a single unit in a HDSL2/SHDSL line. It is indexed by the ifIndex of the HDSL2/SHDSL line.
hdsl2ShdslInventoryTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Index | ENUM | R
.3 | VendorID | OCTET STRING | R
.4 | VendorModelNumber | OCTET STRING | R
.5 | VendorSerialNumber | OCTET STRING | R
.6 | VendorEOCSoftwareVersion | INTEGER | R
.7 | StandardVersion | INTEGER | R
.8 | VendorListNumber | OCTET STRING | R
.9 | VendorIssueNumber | OCTET STRING | R
.10 | VendorSoftwareVersion | OCTET STRING | R
.11 | EquipmentCode | OCTET STRING | R
.12 | VendorOther | OCTET STRING | R
.13 | TransmissionModeCapability | ENUM | R
IfIndex
This object specifies the associated interface index of this HDSL2/SHDSL line.
Index
Each entry in this table corresponds to a physical element in a HDSL2/SHDSL Span. It is based on the EOC unit addressing scheme with reference to the xtuC. Enumerations: xtuC (1) xtuR (2) xru1 (3) xru2 (4) xru3 (5) xru4 (6) xru5 (7) xru6 (8) xru7 (9) xru8 (10)
VendorID
Vendor ID as reported in an Inventory Response message. Length: 8 to 8
VendorModelNumber
Vendor model number as reported in an Inventory Response message. Length: 12 to 12
VendorSerialNumber
Vendor serial number as reported in an Inventory Response message. Length: 12 to 12
VendorEOCSoftwareVersion
Vendor EOC version as reported in a Discovery Response message.
StandardVersion
Version of the HDSL2/SHDSL standard implemented, as reported in an Inventory Response message.
VendorListNumber
Vendor list number as reported in an Inventory Response message. Length: 3 to 3
VendorIssueNumber
Vendor issue number as reported in an Inventory Response message. Length: 2 to 2
VendorSoftwareVersion
Vendor software version as reported in an Inventory Response message. Length: 6 to 6
EquipmentCode
Equipment code conforming to ANSI T1.213, Coded Identification of Equipment Entities. Length: 10 to 10
VendorOther
Other vendor information as reported in an Inventory Response message. Length: 12 to 12
TransmissionModeCapability
Contains the transmission mode capability of the SHDSL unit: region1 - ITU-T G.991.2 Annex A region2 - ITU-T G.991.2 Annex B Enumerations: region1 (1) region2 (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH