>> MIB - Management Information Base
>> Table: pppoeCallTable - (.1.3.6.1.4.1.272.4.24.1.1)
Description: The pppoeCallTable displays all currently active PPPoE calls (incoming and outgoing). Only the system can add or remove entries to this table. Creating entries: Entries are added when an outgoing call is made or when an incoming call is connected. Deleting entries: Entries are removed once the respective call is disconnected.
pppoeCallTable
OID | Name | Type | Access
.1 | Id | INTEGER | R
.2 | Direction | ENUM | R
.3 | Age | TimeTicks | R
.4 | State | ENUM | RW
.5 | RemotePhysAddress | PhysAddress | R
.6 | LocalPhysAddress | PhysAddress | R
.7 | AcName | DisplayString | R
.8 | Service | DisplayString | R
.9 | ReceivedPackets | Counter | R
.10 | ReceivedOctets | Counter | R
.11 | ReceivedErrors | Counter | R
.12 | TransmitPackets | Counter | R
.13 | TransmitOctets | Counter | R
.14 | TransmitErrors | Counter | R
.15 | Info | DisplayString | R
.16 | SessionId | INTEGER | R
.17 | EthIfIndex | INTEGER | R
.18 | AssociatedIfIndex | INTEGER | R
Id
System internal and unique ID for the related PPPoE call.
Direction
Direction of the PPPoE call, incoming(1) or outgoing(2). Enumerations: incoming (1) outgoing (2)
Age
The age of the call. For outgoing calls, the time since the call began, or for incoming calls, the time since the call was received. The format is in hh:mm:ss.00.
State
The state of the PPPoE discovery stage according RFC 2516. Enumerations: idle (1) wait-pado (2) wait-padr (3) wait-pads (4) established (5) terminated (6) close (7) delete (8)
RemotePhysAddress
Peer's Ethernet address.
LocalPhysAddress
Local Ethernet Address.
AcName
The PPPoE access concentrator's name. Length: 0 to 255
Service
The PPPoE service name, indicating the service the Host is requesting. Length: 0 to 255
ReceivedPackets
Count of received valid GRE-encapsulated packets.
ReceivedOctets
Count of received valid Octets.
ReceivedErrors
Count of received invalid GRE-encapsulated packets.
TransmitPackets
Count of transmitted GRE-encapsulated packets.
TransmitOctets
Count of transmitted Octets.
TransmitErrors
Count of transmit errors.
Info
Additional information to identify the PPPoE call Length: 0 to 255
SessionId
The PPPoE session ID, assigned via PPPoE Active Discovery Session-Confirmation (PADS).
EthIfIndex
The interface index (ifIndex) of the associated Ethernet device.
AssociatedIfIndex
The index of the associated virtual interface.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH